Intermediate Clutch Assembly Installation. GMC Truck Export Savana 1999

For 1990-2009 cars

1. Dip all of the intermediate clutch plates in DEXRON®VI transmission fluid.
2. Install the intermediate clutch wave plate (684) with the tangs facing down.

Note: Alternate the clutch plates, starting with the steel clutch plate (4 steel and 4 composite).

3. Install the intermediate clutch plates (631, 632).
4. Install the intermediate clutch backing plate (630).
5. Install the intermediate clutch backing plate retainer ring (629). The opening of the retainer ring (629) should be at the 9 o'clock position.