Shift Shaft and Shift Forks. GMC Truck Export GMC P42 Commercial Chassis 1999

For 1990-2009 cars

• | Clean all the parts in a suitable solvent. Air dry the parts.

• | Inspect the shift shaft for wear or scoring.

• | Inspect the shift shaft forks for wear, scoring, or distortion.

• | Inspect the roll pins for wear or distortion.

• | Inspect the shift shaft socket assembly components for wear or distortion.

• | Replace the worn or distorted parts. Inspect all the mating parts.