Manual Shift Shaft Removal. GMC Truck Export GMC P42 Commercial Chassis 1999

For 1990-2009 cars

Notice: Use a piece of wood or other protective material when you remove the manual shaft pin, to prevent damage to the case.

1. Remove the manual shift shaft pin (709).
2. Remove the manual shift shaft detent lever nut (712).
3. Remove the manual shift shaft (708).
4. Remove the manual shift shaft seal (707).
5. Inspect the manual shift shaft for the following conditions:

• | Damaged flats or threads

• | Burrs

• | Wear

6. Inspect the manual shift shaft pin (709) for tightness.