INTERMITTENT CONNECTION AT ECM PCM/TCM SENSORS OR COMPONENTS. GMC Truck S15 Pickup - 2WD 1991

For 1990-2009 cars

# INTERMITTENT CONNECTION AT ECM PCM/TCM SENSORS OR COMPONENTS

#### SUBJECT: INTERMITTENT CONNECTION AT ECM/PCM/TCM SENSORS OR COMPONENTS

#### MODELS: 1991 LIGHT AND MEDIUM DUTY TRUCKS WITH ECM/PCM/TCM

Some 1991 Light and Medium duty trucks equipped with Electronic Control Modules (ECM) or Powertrain Control Modules (PCM) or Transmission Control Modules (TCM) may experience a condition in which the female terminals (150 series Metri-pack) in certain sensor or component connectors do not make a solid connection to the male terminals in the opposing connectors. This can result in a intermittent connection. The 1991 Driveability & Emissions Manual (X-9136) directs a check of connections anytime an intermittent condition is found.

The following chart lists the component and circuit numbers that may experience this condition.

Component Circuit Description ------------------------ ------- --------------------- Intake Air Temperature 472 IAT signal (IAT) 2.5L only 469 5 volt return (ground)

Coolant Temperature Sensor 410 CTS signal (CTS) 452 5 volt return (ground)

Throttle Position Sensor 417 TPS signal (TPS) 452 5 volt return (ground)

Electronic Spark Timing Module 453 EST Reference low (EST) 424 EST Bypass 430 EST Reference high 423 EST Control

Transmission Vehicle Speed Sensor 821 Speed Signal high (All Auto. & Manual Transmission) 822 Speed Signal low

Transmission Input Speed Sensor 1230 Input Speed Signal low (4L80E only) 1231 Input Speed Signal high

Transmission Output Speed Sensor 1232 Output Speed Sensor high (4L80E with Four Wheel Drive only) 1233 Output Speed Sensor low

If an intermittent condition is found, the following test procedure should be performed.

Insert a new mating male terminal, P/N 12047581 or 12045773, into the female terminal and check for a slight drag when the terminals are separated. Loose terminals without drag should be replaced. If the amount of drag is questionable, remove the terminal from the connector and inspect the termi- nal for the condition shown in FIGURE 1. Replace any terminals found defective with terminal P/N 12047680.

General directions of terminal replacement can be found on pages 3-146 thru 3-147 of the 1991 Driveability and Emissions Manual.

#### Important

Do not attempt to repair a defective terminal. All of the above terminal part numbers are contained in J-38125 or are currently available from GMSPO.

WARRANTY INFORMATION

For vehicles repaired under warranty use:

Labor Operation: T7096

Labor Time: This is a ST (Straight Time) operation which requires time documentation as detailed in the claims processing manual. Zone approval is required beyond .5 hours.

#### NOTE: Labor Operation is coded to base vehicle coverage in the warranty system.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.