WOODY CONVERSION PACKAGE PROCEDURE TO ORDER PARTS. GMC Truck S15 Pickup - 2WD 1984

For 1990-2009 cars

# WOODY CONVERSION PACKAGE PROCEDURE TO ORDER PARTS

#### MODELs: 1984 S-T JIMMYS

The attached information will assist you in ordering conversion kits for the 1984 GMC Woody package.

Part numbers listed are Cars and Concepts, Inc. numbers and not GM part numbers. Conversion kits are available on a C.O.D. basis from:

Cars & Concepts, Inc. Attn: Order Desk 12500 E. Grand River Brighton, MI 48116 Phone: (313) 227-1400 Extension 228 Out of State 1-800-521-9753

RECOMMENDED DECAL APPLICATION INSTRUCTIONS

1. Application surface must be above 65 DEG F. clean and free of oil wax, grease or any foreign matter.

A. DuPont's Prep-Sol 39195, R & H Pre-Cleaner, DX330 or any good quality pre-cleaner must be used on surface pnor to installing decals.

2. Tape all markings in proper position with masking tape, prior to beginning application.

3. Place a strip of masking tape down the center(vertically) of the emblem, exceeding the edges top and bottom by approximately 3".

4. Fold one side of decal away from application surface and peel backing paper away from adhesive side of decal up to tape hinge, cut backing paper away, next to hinge. DO NOT PEEL DECAL AWAY FROM BACKING, PEEL BACKING AWAY FROM DECAL.

5. Fold decal back towards surface, keeping adhesive just off application surface, starting at the masking tape hinge, squeegee the decal down using firm overlapping strokes, working from center out. Remove tape hinge and apply the other half in the same manner.

6. Remove the face mask (surface tape) by slowly peeling it back over itself at 180 DEG angle.

7. Puncture any air pockets or bubbles trapped under the decal with a small pin or needle and press air out.

8. Where decal bridges a seam, cut the decal and force it down into the seam.

9. Resqueegee all decals after premask removal and make sure all edges are down.

G.M.C. Woody Service Part Listing

Item No. Part Number Description --- ----------- ----------- 1 1260051A70 Applique Service 2 1560018D41 Bezel A.C. Duct RH 3 1560019D41 Bezel A.C. Duct LH 4 1560020D41 Bezel Inst. Panel 6 1560021E41 Bezel Heater Control 7 1830008C41 Cable Assy. End Gate Support 8 2650259C41 Decal "G.M.C." Woody 9 4180047A00 H/ware Bag - Mldg. 11 5400228C41 Mldg. Frt. Fndr. RH 12 5400229C41 Mldg. Frt. Fndr. LH 13 5400230C41 Mldg. Door RH 14 5400231C41 Mldg. Door LH 15 5400232C41 Mldg. Qtr. Side RH 16 5400233C41 Mldg. Qtr. Side LH 17 5400234C41 Mldg. Tailgate 18 5750013C41 Name Plate "Woody" 19 6400111E41 Plate - Glove Box Trim 20 6400115D11 Plate Assy. Door Trim LH 21 6400116D11 Plate Assy. Door Trim RH 22 6450011C41 Plug Mldg.

NOTE; Item No. 1 Applique Service is a large rectangular wood grained sheet, sufficient enough to replace any one panel. It is not a die cut part, so it must be trimmed to fit.

Item No. 9 Hardware bag - molding includes enough hardware to remove and replace any wooden panel.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.