CAMPAIGN: STEERING WHEEL IMPROPERLY INSTALLED. GMC Truck S15 Pickup - 4WD 1990

For 1990-2009 cars

# CAMPAIGN: STEERING WHEEL IMPROPERLY INSTALLED

#### MODELS: 1990 S/T 15 (MORAINE TRUCK ASSEMBLY)

The National Traffic and Motor Vehicle Safety Act, as amended, provides that each vehicle which is subject to a recall campaign of this type must be adequately repaired within a reasonable time after the owner has tendered it for repair. A failure to adequately repair within 60 days after tender of a vehicle is prima facie evidence of failure to repair within a reasonable time.

If the condition is not adequately repaired within a reasonable time, the owner may be entitled to an identical or reasonably equivalent vehicle at no charge, or to a refund of the purchase price less a reasonable allowance for depreciation.

To avoid having to provide these burdensome solutions, every effort must be made to promptly schedule appointments with owners and to repair their vehicles as soon as possible. As you will see in reading the attached copy of the letter which is being sent to owners, the owner is being instructed to contact the nearest GMC Zone Office if the dealer does not remedy the condition within five days of the mutually agreed upon service date. If the condition is not remedied within a reasonable time, they are instructed how to contact the National Highway Traffic Safety Administration.

#### DEFECT INVOLVED

General Motors has determined that certain 1990 S/T 15 trucks may have improperly installed steering wheels. The nut attaching the steering wheel may have been insufficiently tightened and a nut retainer may be missing. This could allow the steering wheel to disengage from the steering column. Should this occur while the vehicle is in motion, a vehicle crash could occur without prior warning.

To correct this condition the steering wheel nut and retainer will be reinstalled and the nut retorqued on all involved vehicles.

#### VEHICLES INVOLVED

Involved are certain 1990 S/T 15 trucks built at Moraine Truck Assembly. VIN's and dealer codes are listed below:

#### DEALER VIN

48-50456 1GTCS14Z5L2500735 48-06160 1GTCS14E5L2500747 48-50577 1GTCS14Z5L2500749 48-21484 1GTCS14Z6L2500758 48-06053 1GTDT14Z6L2500759 48-18030 1GTDT19Z2L2500766 48-06237 1GTCS14E7L2500782 48-53395 1GTDT19Z8L2500786 48-53379 1GTCS14Z2L2500806 48-50170 1GTCS14E9L2500816 48-21152 1GTDT19Z4L2500817 48-30347 1GTCS14E2L2500835

The specific vehicles involved in this campaign have been identified by Vehicle Identification Number Computer Listings. These listings are furnished to all involved dealers with the campaign bulletin.

#### DEALER CAMPAIGN RESPONSIBILITY

Dealers are to service all vehicles subject to this campaign at no charge to owners, regardless of mileage, age of vehicle, or ownership, from this time forward. Dealers are to inspect and correct all affected vehicles in new and used vehicle stock prior to their sale.

Whenever a vehicle subject to this campaign is taken into your new or used vehicle inventory, or it is in your dealership for service in the future, you should take the steps necessary to ensure the campaign correction has been made before reselling or releasing the vehicle.

Owners of vehicles recently sold from your new vehicle inventory are to be contacted by the dealer and arrangements made to make the required cor- rection according to instructions contained in this bulletin.

If no owner's name and address were available to GMC Truck Division at the time of campaign initiation, the dealer will determine the owner's name and address from the dealership sales records. Please provide this information directly on the second copy of the listing next to the applicable VIN so that our records may be updated and the appropriate notification mailed to the owner. This second copy should then be submitted to the address listed below in the previously supplied yellow campaign envelopes.

GMC Truck Division General Motors Corporation 101 Union Street Plymouth, Michigan 48170

#### OWNER NOTIFICATION

Owners will be notified of this campaign on their vehicles by GMC Truck Division (see copy of owner letter included with this bulletin). A listing of owner names and addresses has been furnished to the involved dealers to enable dealers to follow up with owners involved in this campaign. This listing may contain owner names and addresses obtained from State Motor Vehicle Registration records. The use of such motor vehicle registration data for any other purpose is a violation of law in several states. Accordingly, you are urged to limit the use of this listing to this campaign.

#### SERVICE PROCEDURE (See Figure 1)

1. Disconnect battery ground cable.

2. Remove the horn cap assembly (2) as shown.

3. Disconnect horn lead connection.

4. Inspect to see that nut retainer (3) is undamaged. Replace if necessary.

5. Check to see that steering wheel nut (4) is properly torqued 35-58 Nm (25-35 lb. ft).

6. Re-install nut retainer (3), reconnect horn lead, horn button, and reconnect negative battery lead.

#### PARTS INFORMATION

Parts are to be obtained from General Motors Service Parts Operation (GMSPO). To ensure that these parts will be obtained as soon as possible, they should be ordered from GMSPO on a C.I.O. order with no special instruction code but order under an advise code (2).

Part Number Description Quantity ------ ----------- -------- 419454 Retainer, Steering Wheel 1 Nut (As Required)

7846970 Nut, Steering Column 1 Shaft (As Reequired)

#### NOTE: Substitutions for above parts are not permitted.

#### WARRANTY INFORMATION

Dealers should submit an accurately filled out Warranty Repair Order on each vehicle completed under this campaign.

LABOR OPERATION TIME TROUBLE NUMBER DESCRIPTION ALLOWANCE CODE ------- ------------ --------- ----

V5870 Inspect and reinstall .2 Hr 96 steering wheel nut and retainer

*For dealer to receive Administrative Time Allowance associated with this campaign, add 0. 1 hour to the Labor Operation Time Allowance.

#### CAMPAIGN IDENTIFICATION LABEL

Each vehicle corrected in accordance with the instructions outlined in this product campaign bulletin will require a "Campaign Identification Label." Each label provides a space to include the five (5) digit dealer code of the dealer performing the campaign service. This information may be inserted with a typewriter or ball point pen.

Each "Campaign Identification Label" is to be located on the radiator core support in an area which will be visible when the vehicle is brought in for periodic servicing by the owner.

Apply "Campaign Identification Label" only on a clean, dry surface.

#### ADMINISTRATIVE PROCEDURE

Procedures covering this campaign are outlined in Section V of your dealership's "GM Truck Claims Processing Manual" P 8919.

Dear GMC Owner:

This notice is sent to you in accordance with the requirements of the National Traffic and Motor Vehide Safety Act.

General Motors has determined that certain 1990 S/T 15 trucks may have improperly installed steering wheels. The nut attaching the steering wheel may have been insufficiently tightened and a nut retainer may be missing. This could allow the steering wheel to disengage from the steering column. Should this occur while the vehicle is in motion, a vehicle crash could occur without prior warning.

To correct this condition the steering wheel nut and retainer will be reinstalled on all involved vehicles. This service will be performed for you at no charge. Instructions for performing this service have been sent to your GMC dealer. Parts are available. Please contact your dealer to arrange a service date. The labor time necessary to perform this correction is approximately 15 minutes. Please ask your dealer how much additional time will be needed to process your vehicle.

Your GMC dealer is best equipped to obtain parts and provide service to ensure your vehicle is corrected as promptly as possible. However, if you take your vehicle to your dealer on the agreed service date and they do not service this condition on that date or within five days, we recommend you contact your nearest GMC Truck Zone Office by telephone. The Zone Office will assist you and your dealer in getting your vehicle corrected. The telephone numbers of the Zone Offices are listed in your Warranty and Owner Assistance Information Manual.

After contacting your dealer and the Zone Office, if you are still not satisfied that we have done our best to remedy this condition without charge within a reasonable time, you may wish to write the Administrator, National Highway Traffic Safety Administration, 400 Seventh Street, S.W., Washington, D.C. 20590, or call 800-424-9393 (Washington, D.C. residents use 366-0123).

The enclosed postage paid owner reply card identifies your vehicle. Presentation of this card to your dealer will assist in making the necessary correction to your vehicle in the shortest possible time. If you have sold or traded your vehicle, please furnish us complete name and address of the person you sold or traded your vehicle to and return the card to US.

We are sorry to cause you this inconvenience; however, we have taken this action in the interest of your safety and continued satisfaction with our products.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.