SMU - REVISED 'D' HEIGHT SPECIFICATIONS. GMC Truck S15 Pickup - 4WD 1984

For 1990-2009 cars

# SMU - REVISED 'D' HEIGHT SPECIFICATIONS

#### SUBJECT: SERVICE MANUAL UPDATE - REVISED "D" HEIGHT SPECIFICATIONS

#### MODELS: 1982-96 CHEVROLET AND GMC TRUCK S/T MODELS 1991-94, 1996 OLDSMOBILE BRAVADA

THIS BULLETIN HAS BEEN ISSUED TO REVISE THE SPECIFICATIONS REFERRING TO THE "D" HEIGHT RANGES.

ALL UTILITY MODELS "D" HEIGHT SPECIFICATION RANGE 130.08MM TO 148.11MM

ALL PICK-UP MODELS "D" HEIGHT SPECIFICATION RANGE 130.7MM TO 161.5MM

FIGURES: 0 ATTACHMENTS: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.