TV CABLE IDENTIFICATION LIST OF TV CABLE CODES 700-R4. GMC Truck S15 Pickup - 4WD 1983

For 1990-2009 cars

# TV CABLE IDENTIFICATION LIST OF TV CABLE CODES 700-R4

1982-1985 LIGHT DUTY WITH 700-R4 AUTOMATIC TRANSMISSIONS

On-vehicle identification of the TV cable may be accomplished by locating the two-letter code imprinted on tape approximately 1-1/2" behind the adjusting mechanism (see Figure No. 1). TV cable application is determined by the engine used in the vehicle.

The following is a list of TV cable codes, part numbers, and applications used in trucks equipped with the 700-R4 automatic transmission.

Engine Cable Code Part Number ------ ---------- ----------- 2.0L AX 25513305 2.5L FT 25517312 2.8L NC 14040597 4.1L FL 25515600 4.3L ON 25522513 5.0L-5.7L FJ 25515598 6.2L FK 25515599

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.