1993 PAINT CODES, SUPPLIERS, ASSY. PLANT ID-(SERVICE INFO). GMC Truck S15 Pickup - 2WD 1993

For 1990-2009 cars

# 1993 PAINT CODES, SUPPLIERS, ASSY. PLANT ID-(SERVICE INFO)

#### SUBJECT: 1993 PAINT CODES, PAINT SUPPLIERS AND ASSEMBLY PLANT IDENTIFICATION (SERVICE INFORMATION)

#### VEHICLES AFFECTED: 1993 TRUCKS

THIS BULLETIN SUPERSEDES AND REPLACES CORPORATE BULLETIN REFERENCE NUMBER 161702R.** THIS BULLETIN IS BEING REVISED FOR 1993 TRUCKS.

#### 1993 ASSEMBLY PLANT PAINT IDENTIFICATION

Attached is a current listing of the various assembly plants and their paint suppliers. It should be noted, however, that paint suppliers are subject to change at any given time.

Paint Type Assembly Plant (Trucks) Code Supplier ---------- ----------------------- ---- -------- Basecoat/Clearcoat Enamel Baltimore, MD (M/L) B PPG High Solids Enamel Janesville, WI (MD) J Dupont Basecoat/Clearcoat Enamel Flint, MI F BASF High Solids Enamel Moraine, OH (S/T) 2 Dupont Basecoat/Clearcoat Waterborne Oshawa Truck Plant (C/K) 1 PPG High Solids Enamel Pontiac-West, MI (S/T) 0 BASF Basecoat/Clearcoat Enamel Pontiac-East, MI (C/K) E Dupont Medium Solids Enamel Scarborough, Ontario (G) 4 PPG High Solids Enamel Shreveport, LA (S/T) 8 BASF Basecoat/Clearcoat Enamel Ft. Wayne, IN (C/K) Z Dupont Baser-oat/Clearcoat Enamel Janesville, WI (C/K - J PPG Surburban, Yukon, Sierra Crew Cab)

I. BASF REFINISHED PAINTS ARE AVAILABLE IN:

o A - Alphacryl(R)

o D - Diamont 88(R)

o SO Diamont Solo(R)

o 21 Glasurit-21(R)

o 54 Glasurit-54(R)

o S - Limco Select(R)

o L - Limco Supreme Gold(R)

o M - Miracryl(R)

o Super Max(R)

#### Flexible Finishes

When spraying flexible plastic parts, use the following recommendation:

Elastifier additive 521-111 for Vinyl application when using Glasurit (R) 54 and 21 lines.

891 Flex Agent for Vinyl Application when using Alphacryl(R), Miracryl(R), Diamont 88(R), and Supreme Gold(R).

DF-25 for Vinyl application when using Diamont Solo(R).

#### NOTE: When using a basecoat/clearcoat system only use the flex agent in the clearcoat application.

#### Stone Chip Protector

Glassohyd(TM) 1109-1240/6 Stone Chip Protector is a waterborne material which uses a durable, flexible plastic dispersion as its bonding media. This product is versatile in application and may be easily applied by spray, brush, or roller. When Glassohyd(TM) is completely cured, the material is resistant to water, gasoline, and oil. Glassohyd(TM) has excellent stone impact and corrosion resistance. Glassohyd(TM) Stone Chip Protector can be topcoated directly with 21-line or 54/94-line colors.

II. DUPONT REFINISHED PAINTS ARE AVAILABLE IN:

o L-Lucite(R) --- Acrylic Lacquer

o A-Centari(R) --- Acrylic Enamel

o J-Cronar(R) --- Polyoxithane Enamel

o K-ChromabaseTM

o 350S--Flexlar(R)---Flexible Additive

o 310S--Black --- 1-2-3 Vinyl Lacquer

o 330S--White --- 1-2-3 Vinyl Lacquer

o V-Lucite Vinyl

#### IMPORTANT: --------- Vinyl resin must be added to the base colour when painting interior components. DuPont vinyl resin 304S (instrument panel).

DuPont vinyl resin 305S (all remaining interior parts except seats).

DuPont vinyl resin 306S (seats and vinyl roofs).

When ordering DuPont paint, use "L", "A", "J", "K", or "V' with the appropriate DuPont Code.

III. PPG (DITZLER) REFINISH PAINTS ARE AVAILABLE IN:

DDL--Duracryl(R) --- Acrylic Lacquer or Acrylic Basecoat/Clearcoat

DBU--Deltron(R) --- Basecoat/Clearcoat

DAR--Delstar(R) --- Acrylic Enamel

DAU--Deltron(R) --- Acrylic Urethane

UCV --- Vinyl Colours

DX-369--Flexative(R)---Flexible Finishes

DX-54--Roadguard(R) --- Road Abrasion Protection

When ordering PPG (Ditzler) paint, use "DDL", "DBU", "DAR", "DAU", "UCV", "DX-54", or "DX-369" with appropriate Ditzler code.

#### BULLETIN REFERENCES:

Corporate Ref. 161702R

General Motors of Canada 92-2-102 Chevrolet Division 92-08-10 GMC Truck Division 92-10-05

#### 1993 TRUCK INTERIOR COLORS

GM COLOR NAME GLOSS FISHER PPG PPG VINYL (BASF) DUPONT TRIM SEMI FLAT W- DIA INTERIOR RINSHED CODE CODE CODE UCV CODE MASON ---------------------------------------------------------------------------- 12DN GRAPHITE X 7701 33622 2-1020 16042 X 7701 33870 2-1020 13199

13AN LT. SM. GRAY X 9653 35203 2-1441 21026 C9109 X 9653 35204 2-1441 21029 C9110

13BN MED. SM. GRAY X 9654 35205 2-1442 21027 C9110

13CN DK. SM. GRAY X 9655 35206 2-1443 21028 C9111

18DN DK. CHARCOAL X 7350 33872 2-871 14030 C8575 X 7350 33492 2-871 12730 C8575

19DN BLACK X 848 9640 2-120 12812 C8535 X 848 9433 2-120 4401 C8535

24CN DK. BLUE X 9059 16323 2-1276 19021 C8792 X 9059 16323 2-1276 17124 C8792

24DN VERY DK. BLUE X 8576 15886 2-1098 16045 C8539 X 8576 16092 2-1098 15080 C8539

24EN MIDNIGHT BLUE X 9541 16998 2-1396 20066 C9006 X 9541 16999 2-1396 20065 C9006

47CN DARK RED X 9104 73381 2-1394 20062 C9007 X 9104 73380 2-1394 20061 C9007

47DN VERY DARK RED X 9253 73383 2-1395 22274 C9008 X 9753 73382 2-1395 20063 C9008

60BN MED. COGNAC X 9205 26281 2-1292 19022 C8808 X 9205 26281 2-1292 18055 C8808

60CN DARK COGNAC X 9099 26284 2-1315 18057 C8810 X 9099 26284 2-1315 18056 C8810

64AN LIGHT BEIGE X 9776 27307 2-1477 22251 C9230 X 9776 27307 2-1477 22276 C9230

64BN MEDIUM BEIGE X 9777 27312 2-1478 22277 C9231 X 9777 27308 2-1478 22278 C9231

64DN DARK BEIGE X 9776 27313 2-1479 22279 C9232 X 9776 27309 2-1479 22280 C9232

#### 1993 TRUCK EXTERIOR COLORS

GM WA COLOR DUPONT AKZO PPG BASF GLASURIT ICI CIL NO. NO. NAME SIKKENS DDI RIN- 54-21 AUTO DAR SHED LINE COLOR MASON ---------------------------------------------------------------------------- 10 9225 GHOST WHITE AE660 GMA86:10 4015 18121 GM-9225 TD26B 40594 13 6111 LINEN WHITE 21667 GMA79:12 2815 1347 GM-5438 HA62 1473 14 8915 GUNMETAL AC547 GMA93:14 3805 15260 GM-8915 1AA7B 42493 15 8914 ASTRAL SILVER AC546 GMA85:15 3796 15251 GM-7054 1897B 39399 T 16 9659 WARM GRAY MET DF243 GMA91:16 4314 21017 GM-9659 C849B 42282 T 17 7466 LT SLATE GRAY AK903 GMA83:17 12866 GM-7023 18 9017 DOVE GRAY DF856 GMA93:18 35567 23020 GM-9017 2RL1B 43032 T 19 5118 LAMP BLACK 78400 GMA78:19 9000/ PKG 21-1240 WV34 8080 9300 20 9790 LT QUASAR BLUE MET DF840 GMA93:20 4714 23004 GM-9790 4PR4B 43060 22 9656 BAHAMA BLUE MET DF242 GMA91:22 4307 21018 GM-9056 C850B 42283 T 23 7154 OCEAN BLUE BR007 GMA80:23 3250 11500 GM-5481 HA61 1840 24 9222 MED. BLLUE MET AD933 GMA87:24 4110 18120 GM-9222 8195M 40952 40952G 40952R 26 9662 PASTEL BLUE DF702 GMA91:26 4308 21019 GM-9662 XP59 42237 27 9264 LT FRENCH BLUE MET AE682 GMA89:27 4146 19031 GM-9264 C140B 1981 1981LR 28 8863 BLK SAPPHIRE MET AD924 GMA93:28 4003 17118 GM-8863 2NY3B 42914 29 7349 DK BLUE BR106 GMA83:29 3362 12283 GM-5039 HV27 37745 33 9207 LT MESA BROWN AD926 GMA89:33 4152 19028 GM-9207 2NY1B 42915 34 9793 LT TEAL MET DF862 GMA92:34 4455 22072 GM-9793 1AC4B 42583 T 36 9828 MED DK TEAL MET DF864 GMA92:36 4347 22073 GM-9828 1AA3B 42521

#### 1993 TRUCK EXTERIOR COLORS

GM WA COLOR NAME DUPONT AKZO PPG BASF GLASURIT ICI CIL NO. NO. SIKKENS DDI- RINSHED 54-21 AUTO DAR MASON LINE COLOR ---------------------------------------------------------------------------- 38 9794 BRIGHT TEAL MET DF836 GMA93:38 4716 22265 GM-9794 2NX9B 42916 39 9792 INDIGO MET DF857 GMA93:39 4717 23006 GM-9792 2NX8B 42917 41 8555 BLACK AB921 GMA91:41 9700 13572 54-1240 2LF4B 39706 T 44 7964 FOREST GREEN MET AH792 GMA85:44 4114 15366 GM-7964 8359M 1947 T 46 7156 DK GREEN BR008 GMA91:45 3255 11505 GM-5482 HA57 1841 T 47 9095 DK BLUE MET DF525 GMA90:47 4251 20052 GM-9095 8393M 41989 48 9096 DK RED DF526 GMA90:48 4239 20053 GM-9096 XE37 41992 50 8624 OLYMPIC WHITE AC301 GMA85:50 3800 15255 GM-8624 TC75B 39402 T 52 9087 KHAKI DF853 GMA92:52 4718 23021 GM-9087 4PR3B 43061 T 54 9831 SPRUCE MET DF861 GMA92:54 4500 22267 GM-9831 1AF5B 42624 57 5400 BEIGE MET DF778 GMA92:57 4346 22271 GM-5400 1AA4B 42496 T 61 8265 TAN AB415 GMA84:61 3686 14241 GM-1074 KF67 43049 71 7753 RED ORANGE AB153 GMA83:71 3463 12884 GM-3046 JD78 38200 72 7475 STANDARD RED AK412 GMA83:72 3464 12885 GM-3047 JD79 38161 74 9260 VICTORY RED AE737 GMA89:74 4154 19030 GM-9030 TA84B 41440 75 8919 RED MET AC557 GMA85:75 1902B 39406 T 76 9154 DK GARNET RED MET AE068 GMA91:76 4002 17117 GM-9154 PA47B 40583 78 8800 MARRON MET AC605 GMA86:78 16117 GM-3091 7997M 1946 T

#### 1993 TRUCK EXTERIOR COLORS

GM WA COLOR NAME DUPONT AKZO PPG BASF GLASURIT ICI CIL NO. NO. SIKKENS DDI RINSHED 54-21 AUTO DAR MASON LINE COLOR ---------------------------------------------------------------------------- 80 9791 MED QUASAR BLUE DF839 GMA93:80 4719 23022 GM-9791 2NW2B 42918 MET T 83 9916 RADISSON RED MET GMA93:83 4720 23023 GM-9916 2NW3B 42919 84 9927 DK HUNT CLUB MET DF842 GMA93:94 4721 23007 GM-9927 2NW4B 42920 90 8798 GRAY MET AC603 GMA86:90 16118 GM-8793 7998M 1944 91 6270 DK ARGENT DF863 GMA92:91 22223 GM-22223 1AC5 42582 T 96 8867 ULTRA SILVER MET AD911 GMA87:96 4023 18112 GM-8867 A975B 1956 97 9658 DK GRAY MET DF244 GMA91:97 4313 21047 GM-0658 C851B 42287 42287LR

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.