WATER PUMP/SEAL LEAKS NEW DESIGN WATER PUMP ASSEMBLY. GMC Truck S15 Pickup - 2WD 1988

For 1990-2009 cars

# WATER PUMP/SEAL LEAKS NEW DESIGN WATER PUMP ASSEMBLY

#### MODELS: 1987-88 S/T MODELS WITH 2.8L ENGINE (VIN CODE R)

Some 1987-88 S/T trucks equipped with a 2.8L engine (VIN Code R) may exhibit a coolant leak from the water pump weep hole while the engine is running.

If customer comments relative to coolant leaks are received and the water pump is diagnosed as the problem, then install a new water pump assembly which incorporates a new design seal. The new design pump has the same overall appearance as the old part.

WATER PUMP AND GASKET ASSEMBLY MODEL SERVICE PART NUMBER

S/T Truck 10120943

For vehicles repaired under warranty, use: Labor Op: J3480 LaborTime: l.Ohr

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.