SERVICE MANUAL UPDATE RWAL DIAGNOSTIC INFORMATION. GMC Truck S15 Pickup - 2WD 1989

For 1990-2009 cars

# SERVICE MANUAL UPDATE RWAL DIAGNOSTIC INFORMATION

#### VEHICLES AFFECTED: 1988-90 C/K, 1989-90 S/T AND M, 1990 R/V AND G WITH RWAL BRAKES

This bulletin should be used to update the diagnostics chart in RWAL update 4WAL PREVIEW MANUAL 15005.05-1 and service manuals listed.

The attached chart (refer to Figure 1) is a revised code 5 diagnostic chart. The revised chart requires a check of wiring and the transfer case switch operation before the control valve is replaced on 4 wheel drive vehicles. The chart also revises code 5 diagnostic information in the following service manuals:

MANUAL VEHICLES

X-8731 1988 C/K X-8931 1989 C/K X-9031 1990 C/K X-9032 1990 R/V AND G X-8929 1989 S/T X-9029 1990 S/T X-8930 1989 M VAN X-9030 1990 M VAN

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.