CONSOLE DOOR MODIFICATION IMPROVED APPEARANCE AND EFFORT. GMC Truck S15 Pickup - 2WD 1983

For 1990-2009 cars

# CONSOLE DOOR MODIFICATION IMPROVED APPEARANCE AND EFFORT

1983-85 S/T TRUCKS AND JIMMYS EQUIPPED WITH RPO D55 CONSOLE

The seat separator console on 1983-85 Jimmys can be modified to improve the appearance of the lid in the closed position and to allow less closure effort. These changes include the addition of a spring under the door middle attaching screw and a new spring at the door compartment stop.

#### SERVICE PROCEDURE

Remove door from console body (see Figure No. 1).

Install two washers, P/N 2077521, and spring, P/N 15544536, under the door center attaching screw on the hinge side. The tab on the spring should point away from the hinge side of the console (see Figure No. 1).

Discard existing spring at the door compartment stop and install spring P/N 15544543 (see Figure No. 1).

Reinstall console door.

#### PARTS INFORMATION

Part Number Description Quantity ----------- ----------- -------- 15544543 Spring 1 15544536 Spring 1 2077521 Washer 2

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.