SIDE DOOR WATER LEAKS (REPLACE WEATHER STRIP). GMC Truck S15 Pickup - 2WD 1994

For 1990-2009 cars

# SIDE DOOR WATER LEAKS (REPLACE WEATHER STRIP)

#### SUBJECT: SIDE DOOR WATER LEAKS (REPLACE WEATHERSTRIP)

#### MODELS 1994 CHEVROLET AND GMC TRUCK S/T PICKUPS

#### CONDITION:

SOME OWNERS MAY COMMENT THAT WATER IS LEAKING INTO THEIR VEHICLE THROUGH THE SIDE DOORS. SYMPTOMS OF THIS CONDITION ARE WET CARPET AND/OR WATER AROUND THE DOOR SILL PLATE.

#### CAUSE:

THIS CONDITION MAY OCCUR IF THE UPPER DOOR SEAL ADHESIVE DOES NOT BRIDGE THE GAP BETWEEN THE ROOF AND THE A-PILLAR VOID. THE SCREW HOLES IN THE A-PILLAR FOR THE WINDSHIELD SIDE REVEAL MOLDING MAY ALSO ALLOW A WATER PATH INTO THE CAB. IN ADDITION, WATER MAY RUN ALONG THE PRIMARY DOOR SEAL AND ENTER THE CARRIER AT THE TRANSITION OF 3-METAL THICKNESS.

#### CORRECTION:

THIS CONDITION MAY BE CORRECTED BY REPLACING THE SIDE DOOR WEATHERSTRIP (FIGURE 1:A). THE NEW WEATHERSTRIP USES THE C/K STYLE CARRIER TO HELP ELIMINATE WATER LEAKS. IT ALSO HAS A REDUCED BULB SIZE TO DECREASE CLOSING EFFORT. THE SERVICE PROCEDURE IS AS FOLLOWS:

1. REMOVE THE EXISTING WEATHERSTRIP BY PULLING IT FROM THE PINCHWELD FLANGE. 2. POSITION THE PREFORMED CORNER OF THE NEW WEATHERSTRIP IN THE UPPER REAR CORNER OF THE DOOR OPENING. 3. PUSH THE WEATHERSTRIP ONTO THE FLANGE, STARTING AT THE PREFORMED CORNER, AND WORKING AROUND THE ENTIRE EDGE OF THE DOOR OPENING.

SERVICE PARTS INFORMATION:

P/N DESCRIPTION QTY 15997028 WEATHERSTRIP ASM - FRONT SIDE DOOR 1 PER DOOR AS NEEDED

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OP DESCRIPTION LABOR TIME C1060 WEATHERSTRIP-ALIGN OR REPLACE-FRONT DOOR (RH) USE PUBLISHED C1061 WEATHERSTRIP ALIGN OR REPLACE-FRONT DOOR (LH) LABOR OPERATION TIME

FIGURES: 1

CAPTIONS: FIGURE 1 - SIDE DOOR WEATHERSTRIP ASM.

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.