USE OF TEFLON SEALANT TAPE. GMC Truck S15 Pickup - 2WD 1983

For 1990-2009 cars

# USE OF TEFLON SEALANT TAPE

#### VEHICLES AFFECTED: 1982-1984 C,K,G,S,T, With Automatic Transmission

The use of Teflon (R) pipe sealant tape is not recommended for sealing transmission pressure test plugs or cooler line fittings. The residual tape that remains after a plug or fitting has been removed is forced inward when the plug or fitting is reinstalled. This fibrous material is then transferred by transmission oil into the system where it can bind valves and block exhaust ports.

The recommended sealer for this application is GM pipe sealant, P/N 992545, or an equivalent such as LocTite pipe sealant with Teflon.

When installing pressure test plugs, care must be exercised in not exceeding the recommended torque limits, as cracked ports may result.

We believe these sources and their equipment to be reliable. There may be additional manufacturers of such equipment. General Motors does not endorse, indicate any preference for, or assume any responsibility for the products or equipment from these firms or for any such items which may be available from other sources.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.