For 1990-2009 cars

### Removal Procedure

1. Remove the rear transmission mount. Refer to Transmission Rear Mount Replacement.
2. Disconnect the intermediate steering shaft from the steering gear.
3. Remove the steering gear to frame bolts.
4. Secure the steering gear upward in order to gain additional clearance.
5. Remove the transmission mount bracket to transmission bolts.
6. Remove the transmission mount bracket from the vehicle.

### Installation Procedure

1. Position the transmission mount bracket to the transmission.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the transmission mount bracket to transmission bolts and tighten to 110 N·m (81 lb ft).
3. Lower the steering gear to the frame.
4. Install the steering gear to frame bolts and tighten to 110 N·m (81 lb ft).
5. Install the intermediate steering shaft to the steering gear.
6. Install the intermediate steering shaft to gear pinch bolt and tighten to 34 N·m (25 lb ft).
7. Install the rear transmission mount. Refer to Transmission Rear Mount Replacement.