For 1990-2009 cars

### Removal Procedure

1. Remove the rear wiper arm. Refer to Rear Window Wiper Arm Replacement .
2. Remove the liftgate lower trim. Refer to Liftgate Trim Panel Replacement .
3. Remove the rear wiper motor bolts.
4. Remove the motor By sliding the pivot shaft out of the rear window grommet.
5. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the rear wiper motor through the rear window grommet.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the wiper motor bolts.

Tighten
Tighten the bolts to 8 N·m (11 lb ft).

4. Install the liftgate trim panel. Refer to Liftgate Trim Panel Replacement .
5. Install the rear wiper arm. Refer to Rear Window Wiper Arm Replacement .