For 1990-2009 cars

### Removal Procedure

1. Siphon the power steering fluid from the fluid reservoir.
2. Remove the reservoir bolts.

Notice: Refer to Power Steering Hose Disconnected Notice in the Preface section.

3. Loosen the hose clamps and remove both hoses from the reservoir.

### Installation Procedure

1. Attach the power steering fluid reservoir to the reservoir bracket.

Notice: Refer to Installing Hoses without Twists or Bends Notice in the Preface section.

2. Connect both hoses to the fluid reservoir and secure the hose clamps.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the fluid reservoir bolts.

Tighten
Tighten the fluid reservoir bolts to 9 N·m (80 lb in).

Notice: Refer to Using Proper Power Steering Fluid Notice in the Preface section.

4. Fill the fluid reservoir with power steering fluid. Refer to Checking and Adding Power Steering Fluid .

Notice: Refer to Air in the Power Steering System Notice in the Preface section.

5. Bleed the system. Refer to Power Steering System Bleeding .
6. Inspect the power steering system for leaks. If there are leaks, correct the cause of the leaks. Refer to Power Steering Fluid Leaks .