For 1990-2009 cars

## Driver Information Center Replacement C100/Long Body

### Removal Procedure

1. Remove the instrument panel center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement .
2. Remove the screws and the driver information bezel.
3. Remove the screws and the driver information center.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the driver information center with the screws.

Tighten
Tighten the driver information center screws to 2 N·m (18 lb in).

2. Install the driver information bezel with the screws.

Tighten
Tighten the driver information bezel screws to 2 N·m (18 lb in).

3. Install the instrument panel center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement .

## Driver Information Center Replacement C105/Short Body

### Removal Procedure

Important: Left - Hand Drive Shown, Right - Hand Drive Similar.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the instrument panel center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement .
3. Remove the radio. Refer to Radio Replacement .
4. Remove the instrument panel center speaker grille panel.
5. Remove the screws and the driver information bezel.
6. Remove the screws and the driver information center.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the driver information center with the screws.

Tighten
Tighten the driver information center screws to 2 N·m (18 lb in).

2. Install the driver information bezel with the screws.

Tighten
Tighten the driver information bezel screws to 2 N·m (18 lb in).

3. Install the instrument panel center speaker grille panel.
4. Install the radio. Refer to Radio Replacement .
5. Install the instrument panel center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement .
6. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .