For 1990-2009 cars

### Removal Procedure

1. Remove the bolt (1) and the seat belt anchor (2) on the floor.
2. Remove the quarter window trim panel.
3. Remove the wheelhouse trim panel.
4. Remove the bolt (1) and the seat belt anchor (2).
5. Remove the bolt (1) and the seat belt retractor (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the seat belt retractor (2) with the bolt (1).

Tighten
Tighten the seat belt retractor bolt to 38 N·m (28 lb ft).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the seat belt anchor (2) with the bolt (1).

Tighten
Tighten the seat belt anchor bolt to 38 N·m (28 lb ft).

3. Install the wheelhouse trim panel.
4. Install the quarter window trim panel.
5. Install the seat belt anchor with the bolt (1)to the floor.

Tighten
Tighten the seat belt anchor bolt to 38 N·m (28 lb ft).