For 1990-2009 cars

### Disassembly Procedure

#### Special Tools

DW-110-030 Engine Overhaul Stand

1. Remove the engine. Refer to Engine Replacement .
2. Remove the flywheel or flexible plate bolts.
3. Remove the flywheel or flexible plate.
4. Mount the engine assembly on the DW-110-030 .
5. Remove the cylinder head. Refer to Cylinder Head Replacement .
6. Remove the oil pan. Refer to Oil Pan Replacement .
7. Remove the crankshaft balancer. Refer to Crankshaft Balancer Replacement .
8. Remove the oil pump. Refer to Oil Pump Replacement .
9. Remove the starter.
10. Remove the generator.
11. Remove the A/C compressor.
12. Remove the A/C compressor and generator bracket.
13. Remove the connecting rod and piston.
14. Remove the engine bed plate.
15. Remove the crankshaft with the rear oil seal ring.
16. Remove the oil nozzle tube.