For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the front upper speaker cover. Refer to Front Upper Speaker Replacement.
3. Gently pry up on the sun sensor to remove it.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Insert and press the sun sensor into position in the dash.
3. Install the front upper speaker cover. Refer to Front Upper Speaker Replacement.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.