For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the water deflector. Refer to Door Water Deflector Replacement .
3. Remove the screws and the front door lock.
4. Disconnect the lock rods.
5. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Connect the lock rods.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the front door lock with the screws.

Tighten
Tighten the front door lock bolt to 10 N·m (89 lb in).

4. Install the water deflector. Refer to Door Water Deflector Replacement .
5. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .