For 1990-2009 cars

1. Remove the 1-2 reverse carrier thrust washer (590).
2. Remove the 1-2 reverse carrier gear assembly (591).
3. Remove the other 1-2 reverse carrier thrust washer (590).
4. Remove the 1-2 reverse internal gear front thrust bearing assembly (593).
5. Remove the 1-2 reverse internal gear (594).
6. Remove the 1-2 reverse internal gear shim (596).
7. Remove the 1-2 reverse internal gear rear thrust bearing assembly (595), from the 1-2 reverse internal gear (594).