For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the left front seat. Refer to Bucket Seat Replacement.
3. Disconnect the electrical connector from the inclination sensor.
4. Remove the inclination sensor from the bracket by sliding the sensor rearward.
5. Remove the bracket by removing the bolts, if needed.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the inclination sensor in the bracket with bolts (1) and tighten to 10 N m (7 lb ft).
2. Install the inclination sensor on the bracket.
3. Connect the connector of inclination sensor.
4. Install the left front seat. Refer to Bucket Seat Replacement.
5. Connect the negative battery cable.