For 1990-2009 cars

## Maintenance Schedule C100/Long Body Europe

Table 1: | Engine
Table 2: | Chassis and Body

#### Engine

Maintenance Item | Maintenance Interval
--- | ---
Kilometers or time in months, whichever comes first
x 1,000 km | 30 | 60 | 90 | 120 | 150 | 180
x 1,000 miles | 18 | 36 | 54 | 72 | 90 | 108
Years | 1 | 2 | 3 | 4 | 5 | 6
Drive Belts (1) | See the remark (1) below
Engine Oil and Engine Oil Filter - 2.4L (2) (3) (14) | See the remark (14)
Engine Oil and Engine Oil Filter - 3.2L/2.0L Diesel (2) (3) (13) | R | R | R | R | R | R
Cooling System Hose and Connections | I | I | I | I | I | I
Engine Coolant (2) (4) | See remark (4) below.
Fuel Filter - 2.4L/3.2L | -- | I | -- | R | -- | I
Fuel Filter - 2.0L Diesel | -- | R | -- | R | -- | R
Fuel Line and Connections | I | I | I | I | I | I
Air Cleaner Element (5) | R | R | R | R | R | R
Spark Plugs - 2.4L (15) | See remark (15) below.
Spark Plugs - 3.2L | I | I | I | R | I | I
Ignition Cable - 2.4L/3.2L | Replace every 96 000 km (60,000 miles).
Evaporative Emission Canister and Vapor Lines | -- | I | -- | I | -- | I
PCV System | I | I | I | I | I | I
Timing Belt - 2.4L (16) | See the remark (16) below.
Timing Belt - 2.0L Diesel (6) | See remark (6) below.

#### Table Symbols:

I--Inspect these items and their related parts. If necessary, correct, clean, replenish, adjust or replace.

R--Replace or change:

#### Remarks:

(1) Drive Belt Inspection

• | 2.4L: Inspect every 30 000 km (18,000 miles) or 2 years and replace 75 000 km (46,000 miles).

• | 3.2L: Inspect every 30 000 km (18,000 miles) or 2 years and replace every 60 000 km (36,000 miles).

• | 2.0L Diesel: Inspect every 30 000 km (18,000 miles) or 2 years and replace every 90 000 km (54,000 miles) or 5 years.

(2) Refer to Fluid and Lubricant Recommendations

(3) If a vehicle is operated under severe conditions: short distance driving, extensive idling or driving in dusty conditions, change engine oil and the filter more frequently than is recommended in the standard maintenance.

(4) Inspect every 30 000 km (18,000 miles) or 1 year and replace every 240 000 km (148,000 miles) or 5 years.

(5) Inspect every 15 000 km (9,000 miles) or 6 months if under dusty driving conditions. If necessary, correct, clean, or replace.

(6) Inspect every 30 000 km (18,000 miles) or 2 years and replace every 90 000 km (54,000 miles) or 6 years.

(13) Change the engine oil immediately if the change oil lamp illuminates in the instruments cluster.

(14) Replace every 15 000 km (9,000 miles) or 1 year.

(15) Inspect every 15 000 km (9,000 miles) or 1 year and replace 45 000 km (27,000 miles) or 2 years.

(16) Inspect every 30 000 km (18,000 miles) or 2 years and replace every 120 000 km (72,000 miles).

#### Chassis and Body

Maintenance Item | Maintenance Interval
--- | ---
Kilometers or time in months, whichever comes first
x 1,000 km | 30 | 60 | 90 | 120 | 150 | 180
x 1,000 miles | 18 | 36 | 54 | 72 | 90 | 108
Months | 1 | 2 | 3 | 4 | 5 | 6
Air Filter (A/C) (7) | See the remark (7) below)
Exhaust Pipes and Mountings | I | I | I | I | I | I
Brake/Clutch Fluid (2) (8) | Change every 4 years
Front Brake Pads and Discs (9) | I | I | I | I | I | I
Rear Brake Pads Discs (9) | I | I | I | I | I | I
Parking Brake | I | I | I | I | I | I
Brake Line and Connections (Including Booster) | I | I | I | I | I | I
Manual Transaxle Fluid, Transfer Case, Rear Differential Leak Check (2) | I | I | I | I | I | I
Chassis and Underbody Bolts and Nuts Tight/Secure | I | I | I | I | I | I
Automatic Transaxle Fluid (2) (10) | See remark (10) below.
Tire Condition and Inflation Pressure (11) | See remark (11) below.
Wheel Alignment (12) | Inspect when abnormal condition is noted.
Steering Wheel and Linkage | I | I | I | I | I | I
Power Steering Fluid and Lines (2) | I | I | I | I | I | I
Drive Shaft Boots | I | I | I | I | I | I
Safety Belts, Buckles and Anchors | I | I | I | I | I | I
Lubricate Locks, Hinges and Hood Latch | I | I | I | I | I | I

#### Table Symbols:

I--Inspect and, if necessary, correct, clean, replenish, adjust or replace.

R--Replace or change:

#### Remarks:

(2) Refer to Fluid and Lubricant Recommendations .

(7) Replace every 15 000 km (9,000 miles) or 1 year. More frequent maintenance is required if under dusty driving conditions.

(8) Change the brake fluid every 2 years if the vehicle is mainly driven under severe conditions:

• | Driving in hilly or mountainous terrain

• | Towing a trailer frequently

(9) More frequent maintenance is required if under severe conditions: short distance driving, extensive idling, frequent low-speed operation in stop and go traffic or driving in dusty conditions.

(10) The transaxle fluid change is not required. Also, routine inspection of the fluid is not required. Transaxle fluid inspection is only required if there is a symptom indicating a concern with the fluid.

(11) Tire condition should be inspected before driving and tire pressure should be checked each time you fill your fuel tank or at least once a month using a tire pressure gauge.

(12) If necessary, rotate and balance wheels.

## Maintenance Schedule C100/Long Body Except Europe

Table 1: | Engine
Table 2: | Chassis and Body

#### Engine

Maintenance Item | Maintenance Interval
--- | ---
Kilometers or time in months, whichever comes first
x 1,000 km | 10 | 20 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100
x 1,000 miles | 6 | 12 | 18 | 24 | 30 | 36 | 42 | 48 | 54 | 60
Months | 6 | 12 | 18 | 24 | 30 | 36 | 42 | 48 | 54 | 60
Drive Belts - 2.4L | -- | -- | I | -- | -- | I | R | -- | -- | I
Drive Belts - 3.2L | -- | -- | I | -- | -- | R | -- | -- | I | --
Drive Belts - 2.0L Diesel | -- | -- | I | -- | -- | I | -- | -- | R | --
Engine Oil and Engine Oil Filter - 2.4L (1) (2) | R | R | R | R | R | R | R | R | R | R
Engine Oil and Engine Oil Filter - 3.2L/2.0L Diesel (11) | See remark (11) below.
Cooling System Hose and Connections | I | I | I | I | I | I | I | I | I | I
Engine Coolant (1) (3) | See remark (3) below.
Fuel Filter - 2.4L/3.2L (14) | -- | -- | -- | I | -- | -- | -- | I | -- | --
Fuel Filter - 2.0L Diesel | -- | -- | -- | -- | -- | R | -- | -- | -- | --
Fuel Line and Connections | -- | I | -- | I | -- | I | -- | I | -- | I
Air Cleaner Element (4) | I | I | I | R | I | I | I | R | I | I
Spark Plugs - 2.4L | -- | I | -- | R | -- | I | -- | R | -- | I
Spark Plugs - 3.2L (12) | -- | -- | I | -- | -- | I | -- | -- | I | --
Ignition Cable - 2.4L/3.2L | Replace every 96 000 km (60,000 miles)
Evaporative Emission Canister and Vapor Lines | -- | -- | -- | I | -- | -- | -- | I | -- | --
PCV System | -- | -- | I | -- | -- | I | -- | -- | I | --
Timing Belt - 2.4L (5) | -- | -- | I | -- | -- | I | -- | -- | I | --
Timing Belt - 2.0L Diesel | -- | -- | I | -- | -- | I | -- | -- | R | --

#### Table Symbols:

I--Inspect these items and their related parts. If necessary, correct, clean, replenish, adjust or replace.

R--Replace or change:

#### Remarks:

(1) Refer to Fluid and Lubricant Recommendations Fluid and Lubricant Recommendations .

(2) If a vehicle is operated under severe conditions: short distance driving, extensive idling or driving in dusty conditions, change engine oil and the filter every 5 000 km (3,000 miles) or 3 months, whichever comes first.

(3) Inspect the engine coolant every 6 months or 10 000 km (6,000 miles) and replace it every 5 years or 240 000 km (150,000 miles).

(4) Inspect the air cleaner element every 5 000 km (3,000 miles) or 3 months if under dusty driving conditions. If necessary, correct, clean, or replace.

(5) 2.4L: Replace every 120 000 km (72,000 miles).

(11) Replace every 30 000 km (18,000 miles) or 1 year.

(12) Replace the spark plugs every 120 000 km (72,000 miles).

(13) Inspect the timing belt every 30 000 km (18,000 miles) replace it every 90 000 km (54,000 miles).

(14) Replace every 140 000 km (84,000 miles).

#### Chassis and Body

Maintenance Item | Maintenance Interval
--- | ---
Kilometers or time in months, whichever comes first
x 1,000 km | 10 | 20 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100
x 1,000 miles | 6 | 12 | 18 | 24 | 30 | 36 | 42 | 48 | 54 | 60
Months | 6 | 12 | 18 | 24 | 30 | 36 | 42 | 48 | 54 | 60
Air Filter (A/C) (6) | R | R | R | R | R | R | R | R | R | R
Exhaust Pipes and Mountings | I | I | I | I | I | I | I | I | I | I
Brake/Clutch Fluid (1) (7) | I | I | I | I | I | R | I | I | I | I
Front Brake Pads and Discs (8) | -- | -- | I | -- | -- | I | -- | -- | I | --
Rear Brake Pads Discs (8) | -- | -- | I | -- | -- | I | -- | -- | I | --
Parking Brake | -- | -- | I | -- | -- | I | -- | -- | I | --
Brake Line and Connections (Including Booster) | I | I | I | I | I | I | I | I | I | I
Manual Transaxle Fluid (1) | I | I | I | I | I | I | I | I | I | I
Chassis and Underbody Bolts and Nuts Tight/Secure | I | I | I | I | I | I | I | I | I | I
Automatic Transaxle Fluid (1) | See remark (14) below.
The Condition and Inflation Pressure (9) | See remark (9) below.
Wheel Alignment (10) | Inspect when abnormal condition is noted
Steering Wheel and Linkage | I | I | I | I | I | I | I | I | I | I
Power Steering Fluid and Lines (1) | I | I | I | I | I | I | I | I | I | I
Drive Shaft Boots | I | I | I | I | I | I | I | I | I | I
Safety Belts, Buckles and Anchors | I | I | I | I | I | I | I | I | I | I
Lubricate Locks, Hinges and Hood Latch | I | I | I | I | I | I | I | I | I | I

#### Table Symbols:

I--Inspect and if necessary correct, clean, replenish, or adjust.

R--Replace or change:

#### Remarks:

(1) Refer to Fluid and Lubricant Recommendations .

(6) More frequent maintenance is required if under dusty driving conditions.

(7) Change the brake fluid every 30 000 km (18,000 miles) or 18 months if the vehicle is mainly driven under severe conditions:

• | Driving in hilly or mountainous terrain, or

• | Towing a trailer frequently

(8) More frequent maintenance is required if under severe conditions: short distance driving, extensive idling, frequent low-speed operation in stop and go traffic or driving in dusty conditions.

(9) Tire condition should be inspected before driving and tire pressure should be checked each time you fill your fuel tank or at least once a month using a tire pressure gage.

(10) If necessary, rotate and balance wheels.

(14) The transaxle fluid change is not required. Also, routine inspection of the fluid is not required. Transaxle fluid inspection is only required if there is a symptom indicating a concern with the fluid.

## Maintenance Schedule C105/Short Body

Table 1: | Engine
Table 2: | Chassis and Body

#### Engine

Maintenance Item | Maintenance Interval
--- | ---
Kilometers or time in months, whichever comes first
x 1,000 km | 30 | 60 | 90 | 120 | 150 | 180
x 1,000 miles | 18 | 36 | 54 | 72 | 90 | 108
Years | 1 | 2 | 3 | 4 | 5 | 6
Drive Belts | See the remark (1) below
Engine Oil and Engine Oil Filter - 2.4L (2) (3) | See the remark (14)
Engine Oil and Engine Oil Filter - 3.2L/2.0L Diesel (2) (3) (13) | R | R | R | R | R | R
Cooling System Hose and Connections | I | I | I | I | I | I
Engine Coolant (2) | See remark (4) below.
Fuel Filter - 2.4L/3.2L | -- | I | -- | R | -- | I
Fuel Filter - 2.0L Diesel | -- | R | -- | R | -- | R
Fuel Line and Connections | I | I | I | I | I | I
Air Cleaner Element (5) | R | R | R | R | R | R
Spark Plugs - 2.4L | See remark (15) below.
Spark Plugs - 3.2L | I | I | I | R | I | I
Ignition Cable - 2.4L/3.2L | Replace every 96 000 km (60,000 miles).
Evaporative Emission Canister and Vapor Lines | -- | I | -- | I | -- | I
PCV System | I | I | I | I | I | I
Timing Belt - 2.4L | See the remark (16) below.
Timing Belt - 2.0L Diesel | See remark (6) below.

#### Table Symbols:

I--Inspect these items and their related parts. If necessary, correct, clean, replenish, adjust or replace.

R--Replace or change:

#### Remarks:

(1) Drive Belt Inspection

• | 2.4L: Inspect every 30 000 km (18,000 miles) or 2 years and replace 75 000 km (46,000 miles).

• | 3.2L: Inspect every 30 000 km (18,000 miles) or 2 years and replace every 60 000 km (36,000 miles).

• | 2.0L Diesel: Inspect every 30 000 km (18,000 miles) or 2 years and replace every 90 000 km (54,000 miles) or 5 years.

(2) Refer to Fluid and Lubricant Recommendations

(3) If a vehicle is operated under severe conditions: short distance driving, extensive idling or driving in dusty conditions, change engine oil and the filter more frequently than is recommended in the standard maintenance.

(4) Inspect every 30 000 km (18,000 miles) or 1 year and replace every 240 000 km (148,000 miles) or 5 years.

(5) Inspect every 15 000 km (9,000 miles) or 6 months if under dusty driving conditions. If necessary, correct, clean, or replace.

(6) Inspect every 30 000 km (18,000 miles) or 2 years and replace every 90 000 km (54,000 miles) or 6 years.

(13) Change the engine oil immediately if the change oil lamp illuminates in the instruments cluster.

(14) Replace every 15 000 km (9,000 miles) or 1 year.

(15) Inspect every 15 000 km (9,000 miles) or 1 year and replace 45 000 km (27,000 miles) or 2 years.

(16) Inspect every 30 000 km (18,000 miles) or 2 years and replace every 120 000 km (72,000 miles).

#### Chassis and Body

Maintenance Item | Maintenance Interval
--- | ---
Kilometers or time in months, whichever comes first
x 1,000 km | 30 | 60 | 90 | 120 | 150 | 180
x 1,000 miles | 18 | 36 | 54 | 72 | 90 | 108
Months | 1 | 2 | 3 | 4 | 5 | 6
Air Filter (A/C) | See the remark (7) below)
Exhaust Pipes and Mountings | I | I | I | I | I | I
Brake/Clutch Fluid (2) (8) | Change every 4 years
Front Brake Pads and Discs (9) | I | I | I | I | I | I
Rear Brake Pads Discs (9) | I | I | I | I | I | I
Parking Brake | I | I | I | I | I | I
Brake Line and Connections (Including Booster) | I | I | I | I | I | I
Manual Transaxle Fluid, Transfer Case, Rear Differential Leak Check (2) | I | I | I | I | I | I
Chassis and Underbody Bolts and Nuts Tight/Secure | I | I | I | I | I | I
Automatic Transaxle Fluid (2) | See remark (10) below.
Tire Condition and Inflation Pressure | See remark (11) below.
Wheel Alignment (12) | Inspect when abnormal condition is noted.
Steering Wheel and Linkage | I | I | I | I | I | I
Power Steering Fluid and Lines (2) | I | I | I | I | I | I
Drive Shaft Boots | I | I | I | I | I | I
Safety Belts, Buckles and Anchors | I | I | I | I | I | I
Lubricate Locks, Hinges and Hood Latch | I | I | I | I | I | I

#### Table Symbols:

I--Inspect and, if necessary, correct, clean, replenish, adjust or replace.

R--Replace or change:

#### Remarks:

(2) Refer to Fluid and Lubricant Recommendations .

(7) Replace every 15 000 km (9,000 miles) or 1 year. More frequent maintenance is required if under dusty driving conditions.

(8) Change the brake fluid every 2 years if the vehicle is mainly driven under severe conditions:

• | Driving in hilly or mountainous terrain

• | Towing a trailer frequently

(9) More frequent maintenance is required if under severe conditions: short distance driving, extensive idling, frequent low-speed operation in stop and go traffic or driving in dusty conditions.

(10) The transaxle fluid change is not required. Also, routine inspection of the fluid is not required. Transaxle fluid inspection is only required if there is a symptom indicating a concern with the fluid.

(11) Tire condition should be inspected before driving and tire pressure should be checked each time you fill your fuel tank or at least once a month using a tire pressure gauge.

(12) If necessary, rotate and balance wheels.