For 1990-2009 cars

### Removal Procedure

Caution: Do not breathe the air through the EVAP component tubes or hoses. The fuel vapors inside the EVAP components may cause personal injury.

1. Remove the evaporative emission (EVAP) canister assembly. Refer to Evaporative Emission Canister Replacement .
2. Loosen the clamp and disconnect the EVAP emission canister vent hose from the EVAP emission canister filter.
3. Remove the EVAP canister emission filter by unclipping the clips from the canister bracket.

### Installation Procedure

1. Install the EVAP emission canister filter to the EVAP emission canister bracket.
2. Connect the EVAP emission canister vent hose to the EVAP emission canister filter.
3. Install the EVAP emission canister assembly. Refer to Evaporative Emission Canister Replacement .