For 1990-2009 cars

### Removal Procedure

1. Remove the brake fluid reservoir-to-master cylinder pins and remove the fluid level sensor by pushing the end of them.
2. Remove the reservoir from the master cylinder.
3. Plug the brake fluid reservoir to prevent brake fluid loss and contamination.

### Installation Procedure

1. Lubricate the new brake fluid reservoir seals with clean brake fluid.
2. Install the brake fluid reservoir seals into the master cylinder body.
3. Install the brake fluid reservoir-to-master cylinder pins and fluid level sensor.
4. Add the brake fluid.
5. Bleed the brake system. Refer to Hydraulic Brake System Bleeding .