For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disable the supplemental inflatable restraints (SIR). Refer to SIR Disabling and Enabling .
2. Remove the front seat assembly. Refer to Bucket Seat Replacement.
3. Remove the screws (2) and the trim cover (1).
4. Disconnect the electrical connectors (1).
5. Remove the bolt (3) and the seat belt buckle pretensioner (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the seat belt buckle pretensioner (2) and secure with bolt (3).

Tighten
Tighten the seat belt retractor bolt to 38 N·m (28 lb ft).

2. Connect the electrical connectors (1).
3. Install the trim cover (1) and secure with the screws (2).
4. Install the front seat assembly. Refer to Bucket Seat Replacement.
5. Enable the SIR. Refer to SIR Disabling and Enabling.