For 1990-2009 cars

#### Rear Drive System/CCM Scan Tool Data List

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition is ON, engine OFF, and vehicle is stationary
Accelerator Pedal Position Sensor | CCM | A/D | D
Battery Volts | CCM | Volts | B+
Est. RDS Coupling Spd. Variation | CCM | RPM | Varies
Estimate Coupling Temperature | CCM | °C | Varies
LF Wheel Speed Sensor | CCM | km/h | 0
LR Wheel Speed Sensor | CCM | km/h | 0
Rear Drive Solenoid Cmd. | CCM | amps | Varies
Rear Drive System Temperature Sensor | CCM | °C | Varies
Rear Drive Torque Command | CCM | N-m | 0-100%
RF Wheel Speed Sensor | CCM | km/h | 0
RR Wheel Speed Sensor | CCM | km/h | 0
Vehicle Speed | CCM | km/h | Varies