For 1990-2009 cars

### Removal Procedure

Note: Left-Hand Drive Shown, Right-Hand Drive Similar.

1. Remove the instrument panel lower left trim. Refer to Instrument Panel Lower Trim Panel Replacement - Left Side.
2. Remove the screws and bolts.
3. Remove the driver knee bolster.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the driver knee bolster with the screws and bolts. Tighten the screws to 2.5 N·m (23 lb in) and tighten the bolts to 20 N·m (15 lb ft).
2. Install the instrument panel lower left trim. Refer to Instrument Panel Lower Trim Panel Replacement - Left Side.