For 1990-2009 cars

## Instrument Cluster Replacement C100/Long Body

### Removal Procedure

1. Remove the instrument cluster trim panel.

Important: Perform the SPO reprogramming when instrument cluster replaced.

2. Remove the screws and the instrument cluster.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the instrument cluster with the screws.

Tighten
Tighten the instrument cluster screws to 2 N·m (18 lb in).

2. Install the instrument cluster trim panel.

## Instrument Cluster Replacement C105/Short Body

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the steering column cover. Refer to Steering Column Trim Covers Replacement .
3. Remove the instrument cluster trim panel.

Important: Perform the SPO reprogramming when instrument cluster replaced.

4. Remove the screws and the instrument cluster.
5. Disconnect the electrical connectors.

### Installation Procedure

1. Connect the electrical connectors.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the instrument cluster with the screws.

Tighten
Tighten the instrument cluster screws to 2 N·m (18 lb in).

3. Install the instrument cluster trim panel.
4. Install the steering column cover. Refer to Steering Column Trim Covers Replacement .
5. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .