For 1990-2009 cars

#### Keyless Control Function

Press LOCK in the transmitter and all the doors (DOOR) will lock and the FLASH light will flash twice (0.3S ON, 0.3S OFF).

Press UNLOCK in the transmitter and all the doors (DOOR) will unlock and the FLASH light will flash once (0.3S ON). When IGN ON or DOOR OPEN, the keyless entry system will be invalid.

#### Central Control Function

1. Input LOCK SW (P13), LOCK (P7) will output 0.35S ± 50 ms.
2. Input UNLOCK SW (P8), UNLOCK (P1) will output 0.35S ± 50 ms.

#### Code Learning Function

Each receiver is equipped with two transmitters when shipped from the factory. The product is provided with a code learning function. If it is necessary to provide the new transmitter, proceed as the following.

• | Enter

| Press IGN (P2) ON -- OFF for 3 times in 5 seconds, enter the next 5 seconds, input LOCK SW (P13) and UNLOCK SW (P8), enter the code learning mode, the FLASH light will flash twice (0.3S ON, 0.3S OFF), the code learning mode will continue for 10 seconds.

• | Code Learning Press

| LOCK and UNLOCK at the same time, each time a code is learned, LOCK (P7) or UNLOCK (P1) will output once.

• | Exit

| Within 10 seconds after entering the code learning mode, the system will exit automatically to the normal mode while the FLASH light will flash twice (0.3S ON, 0.3S OFF). If the IGN (P2) ON is within 10 seconds, the system will exit the code learning mode automatically to the normal mode while the FLASH light will flash twice (0.3S ON, 0.3S OFF).