For 1990-2009 cars

#### Tools Required

• | EN 46106 Flywheel Holding Tool

• | J 38416-2 Crankshaft Button

• | J 41816 Crankshaft Balancer Remover

1. Install the EN 46106 through the starter mounting hole.
2. Remove the crankshaft balancer bolt.
3. Install the J 38416-2 in the nose of the crankshaft.
4. Install the J 41816 in order to remove the crankshaft balancer.
5. Tighten the center bolt of the J 41816 in order to pull the crankshaft balancer off of the crankshaft.
6. Remove the J 41816 from the crankshaft balancer.
7. Remove the EN 46106 .