For 1990-2009 cars

1. Visually inspect the shoe retaining springs for the following conditions:

• | Excessive corrosion

• | Excessive stretching

• | Broken hook ends

• | Twisting or binding

• | Missing

2. Visually inspect the shoe hold down springs for the following conditions:

• | Bent

• | Broken

• | Missing

3. Visually inspect the park brake lever and the strut for the following conditions:

• | Bent

• | Broken

• | Missing

4. Visually inspect the park brake shoe adjuster for the following conditions:

• | Excessive corrosion

• | Broken

• | Binding

• | Missing

5. Replace the park brake hardware with the park brake shoes if necessary. Refer to Parking Brake Shoe Replacement.