For 1990-2009 cars

### Removal Procedure

1. Discharge the A/C (Air Conditioning) system, if equipped.
2. Remove the radiator grille guide and grille. Refer to Grille Replacement.
3. Remove the engine under cover. Refer to Engine Shield Replacement.
4. Remove the hood primary latch support. Refer to Hood Primary Latch Replacement.
5. Remove the charge air cooler inlet/outlet hoses. Refer to Charge Air Cooler Inlet Pipe and Outlet Pipe Replacement.
6. Remove the A/C condenser from the radiator. Refer to Air Conditioning Condenser Replacement.
7. Remove the radiator upper bracket.
8. Remove the charge air cooler bolts.
9. Remove the charge air cooler.

### Installation Procedure

1. Install the charge air cooler to the radiator.
2. Install the charge air cooler bolts.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the radiator upper bracket and tighten.

• | The charge air cooler bolts to 8.5 N·m (75.2 lb in).

• | The radiator upper bracket bolts to 20 N·m (14.8 lb ft).