For 1990-2009 cars

### Removal Procedure

1. Remove the liftgate lower applique. Refer to Liftgate Applique Replacement.
2. Remove the bolt and rear wiper arm park.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the rear wiper arm park with the bolt and tighten to 3 N·m (27 lb in).
2. Install the liftgate lower applique. Refer to Liftgate Applique Replacement.