For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the radiator grille upper cover.
3. Remove the bolts and the headlamp assembly.
4. Disconnect the headlamp assembly electrical connectors.
5. Remove the cap that conceals the headlamp bulb.
6. Disconnect the headlamp bulb electrical connectors.
7. Remove the headlamp bulbs.

### Installation Procedure

1. Install the headlamp bulbs.
2. Connect the headlamp bulb electrical connectors.
3. Install the cap that conceals the headlamp bulbs.
4. Connect the headlamp assembly electrical connectors.

Notice: Refer to Fastener Notice in the Preface section.

5. Install the headlamp assembly with the bolts.

Tighten
Tighten the headlamp assembly bolts to 7 N·m (62 lb in).

6. Install the radiator grille upper cover.
7. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .