For 1990-2009 cars

### Removal Procedure

1. Raise the hood.
2. Remove the wiper arms. Refer to Windshield Wiper Arm Replacement .
3. Remove the air inlet grille panel sealing strip.
4. Remove the air inlet grille panel retaining clips, and the two-piece grille.

### Installation Procedure

1. Install the two-piece grille with the air inlet grille panel retaining clips.
2. Install the air inlet grille panel sealing strip.
3. Install the wiper arms. Refer to Windshield Wiper Arm Replacement .
4. Lower the hood.