For 1990-2009 cars

## Front Bumper Fascia Energy Absorber Replacement C100/Long Body

### Removal Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the retaining clips on the energy absorber.
3. Remove the upper and lower energy absorbers from the front fascia.

### Installation Procedure

1. Install the upper and lower energy absorbers to the front fascia.
2. Install the retaining clips to the energy absorbers.
3. Install the front bumper fascia Refer to Front Bumper Fascia Replacement.

## Front Bumper Fascia Energy Absorber Replacement C105/Short Body

### Removal Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the retaining clips (1) on the energy absorber.
3. Remove the energy absorber (2) from the front fascia.

### Installation Procedure

1. Install the energy absorber (2) to the front fascia.
2. Install the retaining clips (1) to the energy absorbers.
3. Install the front bumper fascia Refer to Front Bumper Fascia Replacement.