For 1990-2009 cars

### Removal Procedure

Important: Use tape around center trim bezel and the end of the flat bladed tool to protect from scratches.

1. Using a flat bladed tool, unfasten the center trim bezel clips from the instrument panel.
2. Remove the center trim bezel from the instrument panel.

### Installation Procedure

1. Position the center trim bezel to the instrument panel.
2. Press the center trim bezel to the instrument panel making sure the clips are fully seated.