For 1990-2009 cars

### Removal Procedure

1. Remove the hood. Refer to Hood Replacement .
2. Remove the fender. Refer to Front Fender Replacement .
3. Remove the bolts and the hinge.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the hinge with the bolts.

Tighten
Tighten the hinge bolts to 24 N·m (18 lb ft).

2. Install the fender. Refer to Front Fender Replacement .
3. Install the hood. Refer to Hood Replacement .