For 1990-2009 cars

### Removal Procedure

1. Remove the bolts securing the rear portion of the 3rd rear seat to the floor.
2. Remove the 3rd rear seat.

### Installation Procedure

1. Install the 3rd rear seat.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the bolts into the rear portion of the 3rd rear seat.

Tighten
Tighten the rear seat-to-floor bolts to 45 N·m (33 lb ft).