For 1990-2009 cars

This master DTC list includes all applicable DTCs in alphanumeric order with descriptors.

DTC | DTC Descriptor | Module That Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
B0000 | Vehicle Speed Information Circuit Plausibility Failure | Radio | DTC B0000
B0012 | Driver Frontal Deployment Loop Stage 1 | SDM | DTC B0012
B0014 | LH Front Side Deployment Loop | SDM | DTC B0014
B0015 | Left Front Seat Belt Pretensioner Deployment Loop | SDM | DTC B0015
B0016 | LH Roof Rail Deployment Loop | SDM | DTC B0016
B0019 | Passenger Frontal Deployment Loop Stage 1 | SDM | DTC B0019
B001A | Left Front/Driver Seat Belt Pretensioner Deployment Loop 2 | SDM | DTC B001A
B001B | Right Front/Passenger Seat Belt Pretensioner Deployment Loop 2 | SDM | DTC B001B
B0021 | RH Front Side Deployment Loop | SDM | DTC B0021
B0022 | Right Front Seat Belt Pretensioner Deployment Loop | SDM | DTC B0022
B0023 | RH Roof Rail Deployment Loop | SDM | DTC B0023
B0052 | Deployment Commanded | SDM | DTC B0052
B0053 | Deployment Commanded With Loop DTCs Present | SDM | DTC B0053
B0055 | Side Air Bag Deployment Commanded | SDM | DTC B0055
B0085 | LF Side Impact Sensor (SIS) | SDM | DTC B0085
B0086 | RF Side Impact Sensor (SIS) | SDM | DTC B0086
B0158 | Outside Air Temperature Sensor Circuit | BCM | DTC B0158
B0163 | Front PCAT Sensor Input Voltage | BCM | DTC B0163, B0173, or B0178
B0173 | Duct Sensor Input Voltage | BCM | DTC B0173 or B0178
B0183 | Front Left Solar Sensor | BCM | DTC B0183
B0193 | Blower Motor Speed | BCM | DTC B0193
B0228 | Air Inlet Door Feedback | BCM | DTC B0228
B0283 | Electric Rear Defrost | BCM | DTC B0283
B0413 | Air Mix Door Feedback | BCM | DTC B0413
B0835 | Cruise Control System Active Indicator Circuit | ECM | DTC B0835
B1000 | Electronic Control Unit (ECU) Performance | BCM | DTC B1000
SDM | DTC B1000
B1001 | Option Configuration Error Variant Not Programmed | BCM | DTC B1001
SDM Option Configuration Error | SDM | DTC B1001
B1015 | VIN Information Error | ECM | DTC B1015
B1016 | VIN Not Programmed | BCM | DTC B1016
Vehicle Identification Number (VIN) Not Programmed | ECM | DTC B1016
B1019 | System Configuration Error | SDM | DTC B1019
B1025 | Audio Output 1 Left Front Circuit | Radio | DTC B1025-B1095
B1035 | Audio Output 2 Right Front Circuit | Radio | DTC B1025-B1095
B1045 | Audio Output 3 Left Rear Circuit | Radio | DTC B1025-B1095
B1055 | Audio Output 4 Right Rear Circuit | Radio | DTC B1025-B1095
B1065 | Audio Output 5 Circuit | Radio | DTC B1025-B1095
B1075 | Audio Output 6 Circuit | Radio | DTC B1025-B1095
B1085 | Audio Output 7 Circuit | Radio | DTC B1025-B1095
B1095 | Audio Output 8 Circuit | Radio | DTC B1025-B1095
B1235 | Amplifier On Signal Circuit | Radio, Amplifier | DTC B1235
B1325 | Device Power Circuit Malfunction | BCM | DTC B1325
B1370 | Device Ignition 1 Circuit | BCM | DTC B1370
SDM | DTC B1370
B1380 | Device Ignition ACCESSORY Circuit | BCM | DTC B1380
B1395 | Voltage Threshold | BCM | DTC B1395
B1428 | Ignition Switched Power Relay 1 Circuit | BCM | DTC B1428
B1433 | Ignition Switched Power Relay 2 Circuit | BCM | DTC B1433
B1440 | Power Mode Master Input Circuits Mismatch | BCM | DTC B1440
B1441 | Device Ignition Off, Run, And Crank Circuit | BCM | DTC B1441
B1475 | Retained Accessory Power Circuit | BCM | DTC B1475
B1517 | Battery Voltage | BCM | DTC B1517
B2494 | Liftgate Handle Switch Circuit | BCM | DTC B2494
B2495 | Liftgate Latch Control Circuit | BCM | DTC B2495
B2530 | Front Fog Lamps Control Circuit | BCM | DTC B2530
B2545 | Backup Lamps Circuit | BCM | DTC B2545
B2575 | Headlamp Control Circuit | BCM | DTC B2575
B257A | Headlamp Switch Input Signals Mismatch | BCM | DTC B257A
B2580 | Headlamp High Beam Control Circuit | BCM | DTC B2580
B2585 | Park Lamp Control Circuit | BCM | DTC B2585
B2625 | Display Dimming Pulse Width Modulation PWM) Output Circuit | BCM | DTC B2625
B2645 | Ambient Light Sensor Circuit | BCM | DTC B2645
B2667 | Control Output | BCM | DTC B2667
B2705 | Gearshift Unlock Circuit | BCM | DTC B2705
B2745 | Traction Control System Circuit Short to Ground | EBCM | DTC B2745
B2750 | Horn Relay Coil Circuit Shorted to Battery | BCM | DTC B2750
B3006 | Hood Ajar Circuit | ECM | DTC B3006
B302A | Telematic Requested Immobilization | ECM | DTC B302A
B3031 | Security System Controller in Learn Mode | ECM | DTC B3031
B3055 | No Transponder Modulation or No Transponder | ECM | DTC B3055
B3060 | Unprogrammed Transponder Identification Code Received | ECM | DTC B3060
B3105 | Keyless Entry System Key Fobs Not Programmed | ECM | DTC B3105
B3109 | Keyless Entry Transmitter 1 or Generic Low Battery | ECM | DTC B3109
B3110 | Keyless Entry Transmitter 2 or Generic Low Battery | ECM | DTC B3110
B3111 | Keyless Entry Transmitter 3 or Generic Low Battery | ECM | DTC B3111
B3112 | Keyless Entry Transmitter 4 or Generic Low Battery | ECM | DTC B3112
B3130 | Passenger Door Unlock Circuit | BCM | DTC B3130
B3135 | All Door Lock Circuit | BCM | DTC B3135
B3265 | Trunk Relay Output | BCM | DTC B3265
B3420 | AHLD Rear Axle Sensor Signal Circuit | BCM | DTC B3420
B3622 | Steering Wheel Controls Group 1 Signal Circuit Voltage Above Threshold | BCM | DTC B3622
B3715 | Front Wiper Relay Drive Circuit | BCM | DTC B3715
B3779 | Mode Door Motor Feedback | BCM | DTC B3779
B3794 | Cruise Control Function Request Circuit | BCM | DTC B3794
B3810 | Headlamp Washer Relay Circuit | BCM | DTC B3810
B3819 | Left Rear Window Up Control Circuit | BCM | DTC B3819
B3820 | Left Rear Window Down Control Circuit | BCM | DTC B3820
B3821 | Left Rear Window Relay Power Circuit | BCM | DTC B3821
B3822 | Right Rear Window Up Control Circuit | BCM | DTC B3822
B3823 | Right Rear Window Down Control Circuit | BCM | DTC B3823
B3824 | Right Rear Window Relay Power Circuit | BCM | DTC B3824
B3843 | Outside Air Quality Sensor Input Voltage | BCM | DTC B3843
B3873 | Front Washer Relay Circuit | BCM | DTC B3873
B3875 | Wiper High Speed Relay Circuit | BCM | DTC B3875
B3887 | Trailer Left Turn Signal Circuit | BCM | DTC B3887
B3888 | Trailer Right Turn Signal Circuit | BCM | DTC B3888
B3891 | Trailer Fog Lamps Circuit | BCM | DTC B3891
B3922 | Front Wiper Function Select Circuit | BCM | DTC B3922
B3933 | Evaporator Temperature Sensor Circuit | BCM | DTC B3933
B3935 | Transponder Authentication Error | ECM | DTC B3935
B3976 | Key Not Programmed | ECM | DTC B3976
C0035 | Left Front Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0040 | Right Front Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0045 | Left Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0050 | Right Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0110 | Pump Motor Circuit | EBCM | DTC C0110
C0131 | ABS/TCS System Pressure Circuit Malfunction | EBCM | DTC C0131
C0161 | ABS Brake Switch Circuit | EBCM | DTC C0161
C0186 | Lateral Accelerometer Circuit | EBCM | DTC C0186
C0196 | Yaw Rate Circuit No Additional Information | EBCM | DTC C0196
C0252 | Steering Wheel Position Sensor Uncorrelated | EBCM | DTC C0252
C0280 | Stability System Active Too Long | EBCM | DTC C0280
C0287 | Longitudinal Accelerometer Circuit | EBCM | DTC C0287
C0292 | VSES Combination Sensor Circuits | EBCM | DTC C0292
C0393 | Rear Axle Coupling Solenoid Control Circuit | BCM | DTC C0393
C0394 | Rear Axle Coupling Temperature Sensor Circuit | BCM | DTC C0394
C0460 | Steering Position Sensor | EBCM | DTC C0460
C0550 | Electronic Control Unit (ECU) Performance | EBCM | DTC C0550
CCM | DTC C0550
C0551 | Option Configuration Error | EBCM | DTC C0551
C0558 | Calibration Mismatch | CCM | DTC C0558
C0561 | System Disabled Information Stored Invalid Serial Data Received | CCM | DTC C0561
EBCM | DTC C0561
C0569 | System Configuration Error | EBCM | DTC C0569
C0750 | Left Front TPMS Transmitter Battery Voltage Too Low | TPMS | DTC C0750, C0755, C0760, or C0765
C0755 | Right Front TPMS Transmitter Battery Voltage Too Low | TPMS | DTC C0750, C0755, C0760, or C0765
C0760 | Left Rear TPMS Transmitter Battery Voltage Too Low | TPMS | DTC C0750, C0755, C0760, or C0765
C0765 | Right Rear TPMS Transmitter Battery Voltage Too Low | TPMS | DTC C0750, C0755, C0760, or C0765
C0899 | Device Power Circuit Low | EBCM | DTC C0899
Device Voltage Low | BCM | DTC C0899
C0900 | Device Power Circuit | EBCM | DTC C0900
P0008 | Engine Position System Performance Bank 1 | ECM | DTC P0008 or P0009
P0009 | Engine Position System Performance Bank 2 | ECM | DTC P0008 or P0009
P0010 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0011 | Intake Camshaft Position (CMP) System Performance Bank 1 | ECM | DTC P0011, P0014, P0021, or P0024
P0013 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0014 | Exhaust Camshaft Position (CMP) System Performance Bank 1 | ECM | DTC P0011, P0014, P0021, or P0024
P0016 | Crankshaft Position (CKP) | ECM | DTC P0016, P0340, or P0341 for the 2.0L engine or DTC P0016, P0017, P0018, or P0019 for the 2.8L, 3.2L, or 3.6L engine
P0017 | Crankshaft Position (CKP) - Exhaust Camshaft Position (CMP) Correlation Bank 1 | ECM | DTC P0016, P0017, P0018, or P0019
P0018 | Crankshaft Position (CKP) - Intake Camshaft Position (CMP) Correlation Bank 2 | ECM | DTC P0016, P0017, P0018, or P0019
P0019 | Crankshaft Position (CKP) - Exhaust Camshaft Position (CMP) Correlation Bank 2 | ECM | DTC P0016, P0017, P0018, or P0019
P0020 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0021 | Intake Camshaft Position (CMP) System Performance Bank 2 | ECM | DTC P0011, P0014, P0021, or P0024
P0023 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0024 | Exhaust Camshaft Position (CMP) System Performance Bank 2 | ECM | DTC P0011, P0014, P0021, or P0024
P0030 | HO2S Heater Control Circuit Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, or P0038 for the 2.4L engine or DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.8L, 3.2L, or 3.6L engine
P0031 | HO2S Heater Control Circuit Low Voltage Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, or P0038 for the 2.4L engine or DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.8L, 3.2L, or 3.6L engine
P0032 | HO2S Heater Control Circuit High Voltage Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, or P0038 for the 2.4L engine or DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.8L, 3.2L, or 3.6L engine
P0036 | HO2S Heater Control Circuit Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, or P0038 for the 2.4L engine or DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.8L, 3.2L, or 3.6L engine
P0037 | HO2S Heater Control Circuit Low Voltage Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, or P0038 for the 2.4L engine or DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.8L, 3.2L, or 3.6L engine
P0038 | HO2S Heater Control Circuit High Voltage Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, or P0038 for the 2.4L engine or DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.8L, 3.2L, or 3.6L engine
P0045 | Turbocharger Boost Control Solenoid Control Circuit | ECM | DTC P0045, P0047, or P0048
P0047 | Turbocharger Boost Control Solenoid Control Circuit Low Voltage | ECM | DTC P0045, P0047, or P0048
P0048 | Turbocharger Boost Control Solenoid Control Circuit High Voltage | ECM | DTC P0045, P0047, or P0048
P0050 | HO2S Heater Control Circuit Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0051 | HO2S Heater Control Circuit Low Voltage Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0052 | HO2S Heater Control Circuit High Voltage Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0053 | HO2S Heater Resistance Bank 1 Sensor 1 | ECM | DTC P0053 or P0059
P0056 | HO2S Heater Control Circuit Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0057 | HO2S Heater Control Circuit Low Voltage Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0058 | HO2S Heater Control Circuit High Voltage Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0059 | HO2S Heater Resistance Bank 2 Sensor 1 | ECM | DTC P0053 or P0059
P0069 | Manifold Absolute Pressure Barometric Pressure Correlation | ECM | DTC P0069
P0087 | Fuel Rail Pressure (FRP) Too Low | ECM | DTC P0087, P0088, or P0089
P0088 | Fuel Rail Pressure (FRP) Too High | ECM | DTC P0087, P0088, or P0089
P0089 | Fuel Pressure Regulator Performance | ECM | DTC P0087, P0088, or P0089
P0090 | Fuel Pressure Regulator Solenoid 1 Control Circuit | ECM | DTC P0090, P0091, or P0092
P0091 | Fuel Pressure Regulator Solenoid 1 Control Circuit Low Voltage | ECM | DTC P0090, P0091, or P0092
P0092 | Fuel Pressure Regulator Solenoid 1 Control Circuit High Voltage | ECM | DTC P0090, P0091, or P0092
P0095 | Intake Air Temperature (IAT) Sensor 2 Circuit Voltage | ECM | DTC P0095, P0097, or P0098
P0097 | Intake Air Temperature (IAT) Sensor 2 Circuit Low Voltage | ECM | DTC P0095, P0097, or P0098
P0098 | Intake Air Temperature (IAT) Sensor 2 Circuit High Voltage | ECM | DTC P0095, P0097, or P0098
P0100 | Mass Air Flow (MAF) Sensor Circuit | ECM | DTC P0100, P0101, P0102, or P0103 for the 2.0L engine or DTC P0100, P0102, or P0103 for the 2.8L, 3.2L, or 3.6L engine
P0101 | Mass Air Flow (MAF) Sensor Circuit Performance | ECM | DTC P0100, P0101, P0102, or P0103 for the 2.0L engine or DTC P0101 for the 2.8L, 3.2L, or 3.6L engine
P0102 | Mass Air Flow (MAF) Sensor Circuit Low Frequency | ECM | DTC P0100, P0101, P0102, or P0103 for the 2.0L engine or DTC P0100, P0102, or P0103 for the 2.8L, 3.2L, or 3.6L engine
P0103 | Mass Air Flow (MAF) Sensor Circuit High Frequency | ECM | DTC P0100, P0101, P0102, or P0103 for the 2.0L engine or DTC P0100, P0102, or P0103 for the 2.8L, 3.2L, or 3.6L engine
P0105 | Manifold Absolute Pressure (MAP) Sensor Circuit | ECM | DTC P0105, P0107, or P0108
P0106 | Manifold Absolute Pressure (MAP) Sensor Performance | ECM | DTC P0106
P0107 | Manifold Absolute Pressure (MAP) Sensor Low Voltage | ECM | DTC P0105, P0107, or P0108 for the 2.0L engine or DTC P0107 or P0108 for the 2.4L engine
P0108 | Manifold Absolute Pressure (MAP) Sensor High Voltage | ECM | DTC P0105, P0107, or P0108 for the 2.0L engine or DTC P0107 or P0108 for the 2.4L engine
P0110 | Intake Air Temperature (IAT) Sensor 1 Circuit Rate of Change | ECM | DTC P0110
P0111 | Intake Air Temperature (IAT) Sensor Circuit Performance | ECM | DTC P0111-P0113
P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | ECM | DTC P0112 or P0113 for the 2.4L engine or DTC P0111-P0113 for the 2.8L, 3.2L, or 3.6L engine
P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage | ECM | DTC P0112 or P0113 for the 2.4L engine or DTC P0111-P0113 for the 2.8L, 3.2L, or 3.6L engine
P0115 | Engine Coolant Temperature (ECT) Sensor Circuit Voltage | ECM | DTC P0115, P0116, P0117, or P0118
P0116 | Engine Coolant Temperature (ECT) Sensor Performance | ECM |

• | DTC P0115, P0116, P0117, or P0118 for the 2.0L engine

• | DTC P0116 for the 2.4L engine

• | DTC P0116 for the 2.8L, 3.2L, or 3.6L engine

P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | ECM |

• | DTC P0115, P0116, P0117, or P0118 for the 2.0L engine

• | DTC P0117 or P0118 for the 2.4L engine

• | DTC P0117 or P0118 for the 2.8L, 3.2L, or 3.6L engine

P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | ECM |

• | DTC P0115, P0116, P0117, or P0118 for the 2.0L engine

• | DTC P0117 or P0118 for the 2.4L engine

• | DTC P0117 or P0118 for the 2.8L, 3.2L, or 3.6L engine

P0119 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent | ECM | DTC P0119
P0121 | Throttle Position (TP) Sensor 1 Performance | ECM | DTC P0121, P0122, P0123, P0221, P0222, P0223, or P2135 for the 2.4L engine or DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.2L, or 3.6L engine
P0122 | Throttle Position (TP) Sensor 1 Circuit Low Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, P0223, or P2135 for the 2.4L engine or DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.2L, or 3.6L engine
P0123 | Throttle Position (TP) Sensor 1 Circuit High Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, P0223, or P2135 for the 2.4L engine or DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.2L, or 3.6L engine
P0125 | Engine Coolant Temperature (ECT) Insufficient for Closed Loop Fuel Control | ECM | DTC P0125
P0128 | Engine Coolant Temperature (ECT) Below Thermostat Regulating Temperature | ECM | DTC P0128
P0130 | HO2S Circuit Closed Loop (CL) Performance Bank 1 Sensor 1 | ECM | DTC P0130 or P0150
P0131 | HO2S Circuit Low Voltage Bank 1 Sensor 1 | ECM | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 2.4L engine or DTC P0131 or P0151 for the 2.8L, 3.2L, or 3.6L engine
P0132 | HO2S Circuit High Voltage Bank 1 Sensor 1 | ECM | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 2.4L engine or DTC P0132 or P0152 for the 2.8L, 3.2L, or 3.6L engine
P0133 | HO2S Slow Response Bank 1 Sensor 1 | ECM | DTC P0133 for the 2.4L engine or DTC P0133 or P0153 for the 2.8L, 3.2L, or 3.6L engine
P0134 | HO2S Circuit Insufficient Activity Bank 1 Sensor 1 | ECM | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 2.4L engine or DTC P0134 or P0154 for the 2.8L, 3.2L, or 3.6L engine
P0135 | HO2S Heater Performance Bank 1 Sensor 1 | ECM | DTC P0135, P0141, P0155, or P0161
P0137 | HO2S Circuit Low Voltage Bank 1 Sensor 2 | ECM | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 2.4L engine or DTC P0137, P0138, P0140, P0157, P0158, or P0160 for the 2.8L, 3.2L, or 3.6L engine
P0138 | HO2S Circuit High Voltage Bank 1 Sensor 2 | ECM | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 2.4L engine or DTC P0137, P0138, P0140, P0157, P0158, or P0160 for the 2.8L, 3.2L, or 3.6L engine
P0140 | HO2S Circuit Insufficient Activity Bank 1 Sensor 2 | ECM | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 2.4L engine or DTC P0137, P0138, P0140, P0157, P0158, or P0160 for the 2.8L, 3.2L, or 3.6L engine
P0141 | HO2S Heater Performance Bank 1 Sensor 2 | ECM | DTC P0135, P0141, P0155, or P0161
P0150 | HO2S Circuit Closed Loop (CL) Performance Bank 2 Sensor 1 | ECM | DTC P0130 or P0150
P0151 | HO2S Circuit High Voltage Bank 2 Sensor 1 | ECM | DTC P0131 or P0151
P0152 | HO2S Circuit Low Voltage Bank 2 Sensor 1 | ECM | DTC P0132 or P0152
P0153 | HO2S Slow Response Bank 2 Sensor 1 | ECM | DTC P0133 or P0153
P0154 | HO2S Circuit Insufficient Activity Bank 2 Sensor 1 | ECM | DTC P0134 or P0154
P0155 | HO2S Heater Performance Bank 2 Sensor 1 | ECM | DTC P0135, P0141, P0155, or P0161
P0157 | HO2S Circuit Low Voltage Bank 2 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0158 | HO2S Circuit High Voltage Bank 2 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0160 | HO2S Circuit Insufficient Activity Bank 2 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0161 | HO2S Heater Performance Bank 2 Sensor 2 | ECM | DTC P0135, P0141, P0155, or P0161
P0180 | Fuel Temperature Sensor Circuit Voltage | ECM | DTC P0180, P0182, or P0183
P0182 | Fuel Temperature Sensor Circuit Low Voltage | ECM | DTC P0180, P0182, or P0183
P0183 | Fuel Temperature Sensor Circuit High Voltage | ECM | DTC P0180, P0182, or P0183
P0190 | Fuel Rail Pressure (FRP) Sensor Circuit | ECM | DTC P0190, P0191, P0192, or P0193
P0191 | Fuel Rail Pressure (FRP) Sensor Performance | ECM | DTC P0190, P0191, P0192, or P0193
P0192 | Fuel Rail Pressure (FRP) Sensor Circuit Low Voltage | ECM | DTC P0190, P0191, P0192, or P0193
P0193 | Fuel Rail Pressure (FRP) Sensor Circuit High Voltage | ECM | DTC P0190, P0191, P0192, or P0193
P0201 | Injector 1 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L engine

• | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine

• | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine

P0202 | Injector 2 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L engine

• | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine

• | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine

P0203 | Injector 3 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L engine

• | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine

• | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine

P0204 | Injector 4 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L engine

• | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine

• | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine

P0205 | Injector 5 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0206 | Injector 6 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0218 | Transmission Fluid Overtemperature | TCM | DTC P0218
P0219 | Engine Overspeed | ECM | DTC P0219
P0221 | Throttle Position (TP) Sensor 2 Performance | ECM | DTC P0121, P0122, P0123, P0221, P0222, P0223, or P2135 for the 2.4L engine or DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.2L, or 3.6L engine
P0222 | Throttle Position (TP) Sensor 2 Circuit Low Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, P0223, or P2135 for the 2.4L engine or DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.2L, or 3.6L engine
P0223 | Throttle Position (TP) Sensor 2 Circuit High Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, P0223, or P2135 for the 2.4L engine or DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.2L, or 3.6L engine
P0234 | Turbocharger Engine Overboost | ECM | DTC P0234 or P0299
P0261 | Injector 1 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0262 | Injector 1 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0263 | Cylinder 1 Balance System | ECM | DTC P0263, P0266, P0269, or P0272
P0264 | Injector 2 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0265 | Injector 2 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0266 | Cylinder 2 Balance System | ECM | DTC P0263, P0266, P0269, or P0272
P0267 | Injector 3 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0268 | Injector 3 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0269 | Cylinder 3 Balance System | ECM | DTC P0263, P0266, P0269, or P0272
P0270 | Injector 4 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0271 | Injector 4 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 2.4L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.2L, or 3.6L engine
P0272 | Cylinder 4 Balance System | ECM | DTC P0263, P0266, P0269, or P0272
P0273 | Injector 5 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0274 | Injector 5 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0276 | Injector 6 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0277 | Injector 6 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0299 | Turbocharger Engine Underboost | ECM | DTC P0234 or P0299
P02E0 | Intake Air (IA) Flow Control Valve Circuit | ECM | DTC P02E0, P02E2, or P02E3
P02E1 | Intake Air (IA) Flow Valve Control Performance | ECM | DTC P02E1
P02E2 | Intake Air (IA) Flow Valve Control Circuit Low Voltage | ECM | DTC P02E0, P02E2, or P02E3
P02E3 | Intake Air (IA) Flow Valve Control Circuit High Voltage | ECM | DTC P02E0, P02E2, or P02E3
P0300 | Engine Misfire Detected | ECM | DTC P0300-P0304 for the 2.4L engine or DTC P0300-P0306 for the 2.8L, 3.2L, or 3.6L engine
P0301 | Cylinder 1 Misfire Detected | ECM | DTC P0300-P0304 for the 2.4L engine or DTC P0300-P0306 for the 2.8L, 3.2L, or 3.6L engine
P0302 | Cylinder 2 Misfire Detected | ECM | DTC P0300-P0304 for the 2.4L engine or DTC P0300-P0306 for the 2.8L, 3.2L, or 3.6L engine
P0303 | Cylinder 3 Misfire Detected | ECM | DTC P0300-P0304 for the 2.4L engine or DTC P0300-P0306 for the 2.8L, 3.2L, or 3.6L engine
P0304 | Cylinder 4 Misfire Detected | ECM | DTC P0300-P0304 for the 2.4L engine or DTC P0300-P0306 for the 2.8L, 3.2L, or 3.6L engine
P0305 | Cylinder 5 Misfire Detected | ECM | DTC P0300-P0306
P0306 | Cylinder 6 Misfire Detected | ECM | DTC P0300-P0306
P0313 | Misfire Detected With Low Fuel Level | ECM | DTC P0313
P0318 | Rough Road Sensor Circuit | ECM | DTC P0318
P0324 | Knock Sensor (KS) Module Performance | ECM | DTC P0324 for the 2.4L engine or DTC P0324 for the 2.8L, 3.2L, or 3.6L engine
P0326 | Knock Sensor (KS) System Performance Bank 1 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0327 | Knock Sensor (KS) Circuit Low Voltage Bank 1 | ECM | DTC P0327 or P0328 for the 2.4L engine or DTC P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.8L, 3.2L, or 3.6L engine
P0328 | Knock Sensor (KS) Circuit High Voltage Bank 1 | ECM | DTC P0327 or P0328 for the 2.4L engine or DTC P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.8L, 3.2L, or 3.6L engine
P0331 | Knock Sensor (KS) System Performance Bank 2 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0332 | Knock Sensor (KS) Circuit Low Voltage Bank 2 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0333 | Knock Sensor (KS) Circuit High Voltage Bank 2 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0335 | Crankshaft Position (CKP) Sensor Circuit | ECM |

• | DTC P0335 or P0336 for the 2.0L engine

• | DTC P0335, P0336, P0337, or P0338 for the 2.4L engine

• | DTC P0335, P0336, or P0338 for the 2.8L, 3.2L, or 3.6L engine

P0336 | Crankshaft Position (CKP) Sensor Circuit Performance | ECM |

• | DTC P0335 or P0336 for the 2.0L engine

• | DTC P0335, P0336, P0337, or P0338 for the 2.4L engine

• | DTC P0335, P0336, or P0338 for the 2.8L, 3.2L, or 3.6L engine

P0337 | Crankshaft Position (CKP) Sensor Circuit Duty Low Cycle | ECM | DTC P0335, P0336, P0337, or P0338
P0338 | Crankshaft Position (CKP) Sensor Circuit Duty High Cycle | ECM | DTC P0335, P0336, P0337, or P0338 for the 2.4L engine or DTC P0335, P0336, or P0338 for the 2.8L, 3.2L, or 3.6L engine
P0340 | Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0016, P0340, or P0341 for the 2.0L engine or DTC P0340, P0341, P0342, or P0343 for the 2.4L engine
P0341 | Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0016, P0340, or P0341 for the 2.0L engine
Intake Camshaft Position (CMP) Sensor Performance Bank 1 | DTC P0340, P0341, P0342, or P0343 for the 2.4L engine
DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393 for the 2.8L, 3.2L, or 3.6L engine
P0342 | Intake Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 1 | ECM | DTC P0340, P0341, P0342, or P0343 for the 2.4L engine or DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393 for the 2.8L, 3.2L, or 3.6L engine
P0343 | Intake Camshaft Position (CMP) Sensor Circuit High Voltage Bank 1 | ECM | DTC P0340, P0341, P0342, or P0343 or DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393 for the 2.8L, 3.2L, or 3.6L engine
P0346 | Intake Camshaft Position (CMP) Sensor Performance Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0347 | Intake Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0348 | Intake Camshaft Position (CMP) Sensor Circuit High Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0350 | Ignition Coil Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0351 | Ignition 1 Coil Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0352 | Ignition 2 Coil Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0353 | Ignition 3 Coil Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0354 | Ignition 4 Coil Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0355 | Ignition 5 Coil Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0356 | Ignition 6 Coil Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0366 | Exhaust Camshaft Position (CMP) Sensor Performance Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0367 | Exhaust Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0368 | Exhaust Camshaft Position (CMP) Sensor Circuit High Voltage Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0391 | Exhaust Camshaft Position (CMP) Sensor Performance Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0392 | Exhaust Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0393 | Exhaust Camshaft Position (CMP) Sensor Circuit High Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0401 | Exhaust Gas Recirculation (EGR) Flow Insufficient | ECM | DTC P0401 or P0402
P0402 | Exhaust Gas Recirculation (EGR) Flow Excessive | ECM | DTC P0401 or P0402
P0403 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit | ECM | DTC P0403, P0489, or P0490 for the 2.0L engine or DTC P0403, P0489, or P0490 for the 2.4L engine
P0404 | Exhaust Gas Recirculation (EGR) Open Position Performance | ECM | DTC P0404, P0405, P0406, P046C, or P049D
P0405 | Exhaust Gas Recirculation (EGR) Position Sensor Circuit Low Voltage | ECM | DTC P0404, P0405, P0406, P046C, or P049D
P0406 | Exhaust Gas Recirculation (EGR) Position Sensor Circuit High Voltage | ECM | DTC P0404, P0405, P0406, P046C, or P049D
P0420 | Catalyst System Low Efficiency Bank 1 | ECM | DTC P0420 for the 2.4L engine or DTC P0420 or P0430 for the 2.8L, 3.2L, or 3.6L engine
P0430 | Catalyst System Low Efficiency Bank 2 | ECM | DTC P0420 or P0430
P0443 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit | ECM | DTC P0443, P0458, or P0459 for the 2.4L engine or DTC P0443, P0458, or P0459 for the 2.8L, 3.2L, or 3.6L engine
P0458 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Low Voltage | ECM | DTC P0443, P0458, or P0459 for the 2.4L engine or DTC P0443, P0458, or P0459 for the 2.8L, 3.2L, or 3.6L engine
P0459 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit High Voltage | ECM | DTC P0443, P0458, or P0459 for the 2.4L engine or DTC P0443, P0458, or P0459 for the 2.8L, 3.2L, or 3.6L engine
P0461 | Fuel Level Sensor 1 Performance | ECM | DTC P0461
P0462 | Fuel Level Sensor 1 Circuit Low Voltage | ECM | DTC P0462
P0463 | Fuel Level Sensor 1 Circuit High Voltage | ECM | DTC P0463
P0480 | Cooling Fan Relay 1 Control Circuit | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0481 | Cooling Fan Relay 2 Control Circuit | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0489 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit Low Voltage | ECM | DTC P0403, P0489, or P0490 for the 2.0L engine or DTC P0403, P0489, or P0490 for the 2.4L engine
P0490 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit High Voltage | ECM | DTC P0403, P0489, or P0490 for the 2.0L engine or DTC P0403, P0489, or P0490 for the 2.4L engine
P0500 | Vehicle Speed Signal (VSS) Circuit | ECM | DTC P0500, P0502, or P0503
P0502 | Vehicle Speed Sensor (VSS) Circuit Low Frequency | ECM | DTC P0500, P0502, or P0503 for the 2.0L engine
P0503 | Vehicle Speed Sensor (VSS) Circuit Intermittent | ECM | DTC P0500, P0502, or P0503 for the 2.0L engine
P0506 | Idle Speed Low | ECM | DTC P0506 or P0507 for the 2.4L engine or DTC P0506 or P0507 for the 2.8L, 3.2L, or 3.6L engine
P0507 | Idle Speed High | ECM | DTC P0506 or P0507 for the 2.4L engine or DTC P0506 or P0507 for the 2.8L, 3.2L, or 3.6L engine
P0513 | Theft Deterrent Key Incorrect | ECM | DTC P0513
P0520 | Engine Oil Pressure (EOP) Switch Circuit | ECM | DTC P0520
P0532 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit Low Voltage | ECM | DTC P0532 or P0533
P0533 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit High Voltage | ECM | DTC P0532 or P0533
P0544 | Exhaust Gas Temperature (EGT) Sensor 1 Circuit | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033
P0545 | Exhaust Gas Temperature (EGT) Sensor 1 Circuit Low Voltage | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033
P0546 | Exhaust Gas Temperature (EGT) Sensor 1 Circuit High Voltage | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033
P0562 | System Voltage Low | ECM | DTC P0562
TCM | DTC P0562 or P0563 for the 6T40/6T45 transmission or DTC P0562 or P0563 for the AF33-5 transmission
P0563 | System Voltage High | ECM | DTC P0563
TCM | DTC P0562 or P0563 for the 6T40/6T45 transmission or DTC P0562 or P0563 for the AF33-5 transmission
P0571 | Brake Switch Circuit 1 | ECM | DTC P0571
P0601 | Control Module Read Only Memory (ROM) | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine

Transmission Control Module (TCM) Read Only Memory (ROM) | TCM | DTC P0601-P0604 or P062F for the 6T40/6T45 transmission or DTC P0601, P0602, P0603, or P0604 for the AF33-5 transmission
P0602 | Control Module Not Programmed | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine

Transmission Control Module (TCM) Not Programmed | TCM | DTC P0601-P0604 or P062F for the 6T40/6T45 transmission or DTC P0601, P0602, P0603, or P0604 for the AF33-5 transmission
P0603 | Control Module Long Term Memory Reset | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine

Transmission Control Module (TCM) Long Term Memory Reset | TCM | DTC P0601-P0604 or P062F for the 6T40/6T45 transmission or DTC P0601, P0602, P0603, or P0604 for the AF33-5 transmission
P0604 | Control Module Random Access Memory (RAM) | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine

Transmission Control Module (TCM) Random Access Memory (RAM) | TCM | DTC P0601-P0604 or P062F for the 6T40/6T45 transmission or DTC P0601, P0602, P0603, or P0604 for the AF33-5 transmission
P0606 | Control Module Internal Performance | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.4L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine

P0607 | Control Module Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F
P060A | Control Module Monitoring Processor Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F
P060B | Control Module Analog to Digital Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F
P0615 | Starter Relay Control Circuit | ECM | DTC P0615
P0616 | Starter Relay Control Circuit Low Voltage | ECM | DTC P0616
P0617 | Starter Relay Control Circuit High Voltage | ECM | DTC P0617
P061C | Control Module Engine Speed Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F
P0621 | Generator L-Terminal Circuit | ECM | DTC P0621
P0625 | Generator F-Terminal Low Voltage | ECM | DTC P0625
P0626 | Generator F-Terminal High Voltage | ECM | DTC P0626
P0627 | Fuel Pump Relay Control Circuit | ECM |

• | DTC P0627 for the 2.0L engine

• | DTC P0627, P0628, or P0629 for the 2.4L engine

• | DTC P0627, P0628, or P0629 for the 2.8L, 3.2L, or 3.6L engine

P0628 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P0627, P0628, or P0629 for the 2.4L engine or DTC P0627, P0628, or P0629 for the 2.8L, 3.2L, or 3.6L engine
P0629 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P0627, P0628, or P0629 for the 2.4L engine or DTC P0627, P0628, or P0629 for the 2.8L, 3.2L, or 3.6L engine
P062B | Control Module Fuel Injector Control Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F
P062F | Control Module Long Term Memory Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F
Transmission Control Module (TCM) Long Term Memory Performance | TCM | DTC P0601-P0604 or P062F
P0630 | VIN Not Programmed or Mismatched - Engine Control Module (ECM) | ECM | DTC P0630 for the 2.0L engine or DTC P0630 for the 2.4L engine
P0633 | Theft Deterrent Key Not Programmed | ECM | DTC P0633
P0634 | Transmission Control Module (TCM) Overtemperature | TCM | DTC P0634
P0638 | Throttle Actuator Control (TAC) Command Performance | ECM | DTC P0638, P2100, P2101, or P2119 for the 2.4L engine or DTC P0638, P2100, P2101, or P2119 for the 2.8L, 3.2L, or 3.6L engine
P0641 | 5-Volt Reference 1 Circuit | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L engine or DTC P0641, P0651, or P0697 for the 2.8L, 3.2L, or 3.6L engine
P0642 | 5-Volt Reference 1 Circuit Low Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0643 | 5-Volt Reference 1 Circuit High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0645 | Air Conditioning (A/C) Clutch Relay Control Circuit | ECM | DTC P0645, P0646, or P0647
P0646 | Air Conditioning (A/C) Clutch Relay Control Circuit Low Voltage | ECM | DTC P0645, P0646, or P0647
P0647 | Air Conditioning (A/C) Clutch Relay Control Circuit High Voltage | ECM | DTC P0645, P0646, or P0647
P064C | Glow Plug Control Module Performance | ECM | DTC P064C
P0650 | Malfunction Indicator Lamp (MIL) Control Circuit | ECM | DTC P0650
P0651 | 5-Volt Reference 2 Circuit | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L engine or DTC P0641, P0651, or P0697 for the 2.8L, 3.2L, or 3.6L engine
P0652 | 5-Volt Reference 2 Circuit Low Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0653 | 5-Volt Reference 2 Circuit High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0658 | Pressure Control (PC)/Shift Lock Solenoid Control Circuit Low Voltage | TCM | DTC P0658 or P0659
P0659 | Pressure Control (PC)/Shift Lock Solenoid Control Circuit High Voltage | TCM | DTC P0658 or P0659
P0667 | Transmission Control Module (TCM) Temperature Sensor Performance | TCM | DTC P0667, P0668, or P0669
P0668 | Transmission Control Module (TCM) Temperature Sensor Circuit Low Voltage | TCM | DTC P0667, P0668, or P0669
P0669 | Transmission Control Module (TCM) Temperature Sensor Circuit High Voltage | TCM | DTC P0667, P0668, or P0669
P0670 | Glow Plug Control Module Control Circuit | ECM | DTC P0670
P0671 | Glow Plug 1 Control Circuit | ECM | DTC P0671, P0672, P0673, or P0674
P0672 | Glow Plug 2 Control Circuit | ECM | DTC P0671, P0672, P0673, or P0674
P0673 | Glow Plug 3 Control Circuit | ECM | DTC P0671, P0672, P0673, or P0674
P0674 | Glow Plug 4 Control Circuit | ECM | DTC P0671, P0672, P0673, or P0674
P0683 | Glow Plug Control Module Communication Circuit | ECM | DTC P0683
P0685 | Engine Controls Ignition Relay Control Circuit | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0686 | Engine Controls Ignition Relay Control Circuit Low Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0687 | Engine Controls Ignition Relay Control Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0689 | Engine Controls Ignition Relay Feedback Circuit Low Voltage | ECM | DTC P0689 for the 2.4L engine or DTC P0685, P0686, P0687, P0689, or P0690 for the 2.8L, 3.2L, or 3.6L engine
P068A | Engine Controls Ignition Relay Control Circuit | ECM | DTC P068A, P068B, or P2510
P068B | Engine Controls Ignition Relay Control Circuit | ECM | DTC P068A, P068B, or P2510
P0690 | Engine Controls Ignition Relay Feedback Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0691 | Cooling Fan Relay 1 Control Circuit Low Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0692 | Cooling Fan Relay 1 Control Circuit High Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0693 | Cooling Fan Relays 2 Control Circuit Low Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0694 | Cooling Fan Relays 2 Control Circuit High Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0697 | 5-Volt Reference 3 Circuit | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.0L engine or DTC P0641, P0651, or P0697 for the 2.8L, 3.2L, or 3.6L engine
P0698 | 5-Volt Reference 3 Circuit Low Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0699 | 5-Volt Reference 3 Circuit High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P06AC | Transmission Control Module (TCM) Power Up Temperature Sensor Performance | TCM | DTC P06AC, P06AD, or P06AE
P06AD | Transmission Control Module (TCM) Power Up Temperature Sensor Circuit Low Voltage | TCM | DTC P06AC, P06AD, or P06AE
P06AE | Transmission Control Module (TCM) Power Up Temperature Sensor Circuit High Voltage | TCM | DTC P06AC, P06AD, or P06AE
P0700 | Transmission Control Module (TCM) Requested MIL Illumination | ECM |

• | DTC P0700 for the 2.0L engine

• | DTC P0700 for the 2.4L engine

• | DTC P0700 for the 2.8L, 3.2L, or 3.6L engine

P0706 | Transmission Range (TR) Switch Performance | TCM | DTC P0706-P0708
P0707 | Transmission Range (TR) Switch Circuit Low Voltage | TCM | DTC P0706-P0708
P0708 | Transmission Range (TR) Switch Circuit High Voltage | TCM | DTC P0706-P0708
P0711 | Transmission Fluid Temperature (TFT) Sensor Performance | TCM | DTC P0711, P0712, or P0713 for the 6T40/6T45 transmission or DTC P0711, P0712, or P0713 for the AF33-5 transmission
P0712 | Transmission Fluid Temperature (TFT) Sensor Circuit Low Voltage | TCM | DTC P0711, P0712, or P0713 for the 6T40/6T45 transmission or DTC P0711, P0712, or P0713 for the AF33-5 transmission
P0713 | Transmission Fluid Temperature (TFT) Sensor Circuit High Voltage | TCM | DTC P0711, P0712, or P0713 for the 6T40/6T45 transmission or DTC P0711, P0712, or P0713 for the AF33-5 transmission
P0716 | Input Speed Sensor Performance | TCM | DTC P0716 or P0717
P0717 | Input Speed Sensor Circuit Low Voltage | TCM | DTC P0716 or P0717 for the 6T40/6T45 transmission or DTC P0717 or P0722 for the AF33-5 transmission
P071D | Trans Mode Switch B circuit | TCM | DTC P071D
P0722 | Output Speed Sensor Circuit Low Voltage | TCM | DTC P0722 or P0723 for the 6T40/6T45 transmission or DTC P0717 or P0722 for the AF33-5 transmission
P0723 | Output Speed Sensor Circuit High Voltage | TCM | DTC P0722 or P0723
P0730 | Incorrect Gear Ratio | TCM | DTC P0730
P0731 | Incorrect 1st Gear Ratio | TCM | DTC P0731
P0732 | Incorrect 2nd Gear Ratio | TCM | DTC P0732
P0733 | Incorrect 3rd Gear Ratio | TCM | DTC P0733
P0734 | Incorrect 4th Gear Ratio | TCM | DTC P0734
P0735 | Incorrect 5th Gear Ratio | TCM | DTC P0735
P0736 | Incorrect Reverse Gear Ratio | TCM | DTC P0736
P0741 | Torque Converter Clutch (TCC) System - Stuck OFF | TCM | DTC P0741 or P0742 for the 6T40/6T45 transmission or DTC P0742 for the AF33-5 transmission
P0742 | Torque Converter Clutch (TCC) System - Stuck ON | TCM | DTC P0741 or P0742 for the 6T40/6T45 transmission or DTC P0742 for the AF33-5 transmission
P0751 | Shift Solenoid (SS) 1 Valve Performance - Stuck Off | TCM | DTC P0751
P0752 | Shift Solenoid (SS) 1 Valve Performance - Stuck On | TCM | DTC P0752
P0762 | Shift Solenoid (SS) 3 Valve Performance Stuck On | TCM | DTC P0762
P0776 | Clutch Pressure Control (PC) Solenoid 2 - Stuck Off | TCM | DTC P0776 or P0777
P0777 | Clutch Pressure Control (PC) Solenoid 2 - Stuck On | TCM | DTC P0776 or P0777
P0796 | Clutch Pressure Control (PC) Solenoid 3 - Stuck Off | TCM | DTC P0796 or P0797
P0797 | Clutch Pressure Control (PC) Solenoid 3 - Stuck On | TCM | DTC P0796 or P0797
P0800 | Active Transfer Case (ATC) Control Module Requested MIL Illumination | ECM | DTC P0800 for the 2.0L engine or DTC P0800 for the 2.4L engine
P0815 | Upshift Switch Circuit | TCM | DTC P0815, P0816, or P0826
P0816 | Downshift Switch Circuit | TCM | DTC P0815, P0816, or P0826
P081A | Starter Inhibit Circuit Low Voltage | TCM | DTC P081A or P081B
P081B | Starter Inhibit Circuit High Voltage | TCM | DTC P081A or P081B
P0826 | Up and Down Shift Switch Circuit | TCM | DTC P0815, P0816, or P0826
P0851 | Park/Neutral Position (PNP) Switch Circuit Low Voltage | TCM | DTC P0851 or P0852
P0852 | Park/Neutral Position (PNP) Switch Circuit High Voltage | TCM | DTC P0851 or P0852
P0856 | Traction Control Torque Request Circuit | ECM | DTC P0856
P0897 | Transmission Fluid Life | TCM | DTC P0897
P0961 | Line Pressure Control (PC) Solenoid Control Circuit Performance | TCM | DTC P0961-P0963
P0962 | Line Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0961-P0963 for the 6T40/6T45 transmission or DTC P0962, P0963, P0966, P0967, P0970, or P0971 for the AF33-5 transmission
P0963 | Line Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0961-P0963 for the 6T40/6T45 transmission or DTC P0962, P0963, P0966, P0967, P0970, or P0971 for the AF33-5 transmission
P0965 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit Performance | TCM | DTC P0965-P0967
P0966 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0965-P0967 for the 6T40/6T45 transmission or DTC P0962, P0963, P0966, P0967, P0970, or P0971 for the AF33-5 transmission
P0967 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0965-P0967 for the 6T40/6T45 transmission or DTC P0962, P0963, P0966, P0967, P0970, or P0971 for the AF33-5 transmission
P0969 | Shift Pressure Control (PC) Solenoid Control Circuit Performance | TCM | DTC P0969-P0971
P0970 | Shift Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0969-P0971 for the 6T40/6T45 transmission or DTC P0962, P0963, P0966, P0967, P0970, or P0971 for the AF33-5 transmission
P0971 | Shift Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0969-P0971 for the 6T40/6T45 transmission or DTC P0962, P0963, P0966, P0967, P0970, or P0971 for the AF33-5 transmission
P0973 | Shift Solenoid (SS) 1 Control Circuit Low Voltage | TCM | DTC P0973 or P0974 for the 6T40/6T45 transmission or DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986 for the AF33-5 transmission
P0974 | Shift Solenoid (SS) 1 Control Circuit High Voltage | TCM | DTC P0973 or P0974 for the 6T40/6T45 transmission or DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986 for the AF33-5 transmission
P0976 | Shift Solenoid (SS) 2 Control Circuit Low Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0977 | Shift Solenoid (SS) 2 Control Circuit High Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0979 | Shift Solenoid (SS) 3 Control Circuit Low Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0980 | Shift Solenoid (SS) 3 Control Circuit High Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0982 | Shift Solenoid (SS) 4 Control Circuit Low Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0983 | Shift Solenoid (SS) 4 Control Circuit High Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0985 | Shift Solenoid (SS) 5 Control Circuit Low Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P0986 | Shift Solenoid (SS) 5 Control Circuit High Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, P0980, P0982, P0983, P0985, or P0986
P1011 | Intake Camshaft Position (CMP) Actuator Park Position Bank 1 | ECM | DTC P1011-P1014
P1012 | Exhaust Camshaft Position (CMP) Actuator Park Position Bank 1 | ECM | DTC P1011-P1014
P1013 | Intake Camshaft Position (CMP) Actuator Park Position Bank 2 | ECM | DTC P1011-P1014
P1014 | Exhaust Camshaft Position (CMP) Actuator Park Position Bank 2 | ECM | DTC P1011-P1014
P1138 | HO2S Circuit High Voltage During Decel Fuel Cut Off (DFCO) Sensor | ECM | DTC P1138
P1224 | Fuel Injector 1 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233
P1227 | Fuel Injector 2 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233
P122A | Fuel Injector 3 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233
P1233 | Fuel Injector 4 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233
P1446 | Pre-catalyst Temperature Too Low During Regeneration | ECM | DTC P1446, P1447, P244C, or P244D
P1447 | Pre-catalyst Temperature Too High During Regeneration | ECM | DTC P1446, P1447, P244C, or P244D
P1551 | Throttle Valve Rest Position Not Reached During Learn | ECM | DTC P1551 for the 2.4L engine or DTC P1551 for the 2.8L, 3.2L, or 3.6L engine
P161C | Tire Size Not Programmed | ECM | DTC P161C
P161E | Glow Plug Positive Voltage Circuit | ECM | DTC P161E
P161F | Assembly Plant Mode Counter Not Programmed | ECM | DTC P161F
P1629 | Theft Deterrent Fuel Enable Signal Not Received | ECM | DTC P1629
P1631 | Theft Deterrent Fuel Enable Signal Not Correct | ECM | DTC P1631
P1632 | Theft Deterrent Fuel Disable Signal Received | ECM | DTC P1632
P1668 | Generator L-Terminal Control Circuit | ECM | DTC P1668
P1682 | Ignition 1 Switch Circuit 2 | ECM | DTC P1682
P1719 | Incorrect Shifting Detected | TCM | DTC P1719
P1751 | Shift Valve 1 Performance | TCM | DTC P1751
P1761 | Tap Up and Down Switch Signal Circuit | TCM | DTC P1761 or P1762
P1762 | Trans Mode Switch Signal Circuit | TCM | DTC P1761 or P1762
P1763 | Trans Mode Switch C Circuit | TCM | DTC P1763
P1793 | Wheel Speed Signal (Invalid Serial Data Received) | ECM | DTC P1793
P1845 | Torque Limit Management | ECM | DTC P1845
P1876 | Up and Down Shift Enable Switch Circuit Low Voltage | TCM | DTC P1876
P2002 | Diesel Particulate Filter Low Efficiency | ECM | DTC P2002
P2008 | Intake Manifold Runner Control (IMRC) Solenoid Control Circuit | ECM | DTC P2008, P2009, or P2010
P2009 | Intake Manifold Runner Control (IMRC) Solenoid Control Circuit Low Voltage | ECM | DTC P2008, P2009, or P2010
P2010 | Intake Manifold Runner Control (IMRC) Solenoid Control Circuit High Voltage | ECM | DTC P2008, P2009, or P2010
P2031 | Exhaust Gas Temperature (EGT) Sensor 2 Circuit | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033
P2032 | Exhaust Gas Temperature (EGT) Sensor 2 Circuit Low Voltage | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033
P2033 | Exhaust Gas Temperature (EGT) Sensor 2 Circuit High Voltage | ECM | DTC P0544, P0545, P0546, P2031, P2032, or P2033
P2066 | Fuel Level Sensor 2 Performance | ECM | DTC P2066
P2067 | Fuel Level Sensor 2 Circuit Low Voltage | ECM | DTC P2067
P2068 | Fuel Level Sensor 2 Circuit High Voltage | ECM | DTC P2068
P2076 | Intake Manifold Tuning (IMT) Valve Position Sensor Performance | ECM | DTC P2076, P2077, or P2078
P2077 | Intake Manifold Tuning (IMT) Valve Position Sensor Circuit Low Voltage | ECM | DTC P2076, P2077, or P2078
P2078 | Intake Manifold Tuning (IMT) Valve Position Sensor Circuit High Voltage | ECM | DTC P2076, P2077, or P2078
P2080 | Exhaust Gas Temperature (EGT) Sensor 1 | ECM | DTC P2080 or P2084
P2084 | Exhaust Gas Temperature (EGT) Sensor 2 | ECM | DTC P2080 or P2084
P2088 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2089 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2090 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2091 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2092 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2093 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2094 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2095 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2096 | Post Catalyst Fuel Trim System Low Limit Bank 1 | ECM | DTC P2096 for the 2.4L engine or DTC P2096 or P2098 for the 2.8L, 3.2L, or 3.6L engine
P2097 | Post Catalyst Fuel Trim System High Limit Bank 1 | ECM | DTC P2097 for the 2.4L engine or DTC P2097 or P2099 for the 2.8L, 3.2L, or 3.6L engine
P2098 | Post Catalyst Fuel Trim System Low Limit Bank 2 | ECM | DTC P2096 or P2098
P2099 | Post Catalyst Fuel Trim System High Limit Bank 2 | ECM | DTC P2097 or P2099
P20E2 | Exhaust Gas Temperature (EGT) Sensor 1-2 Correlation | ECM | DTC P20E2
P2100 | Throttle Actuator Control (TAC) Motor Control Circuit | ECM | DTC P0638, P2100, P2101, or P2119 for the 2.4L engine or DTC P0638, P2100, P2101, or P2119 for the 2.8L, 3.2L, or 3.6L engine
P2101 | Control Module Throttle Actuator Position Performance | ECM | DTC P0638, P2100, P2101, or P2119 for the 2.4L engine or DTC P0638, P2100, P2101, or P2119 for the 2.8L, 3.2L, or 3.6L engine
P2105 | Throttle Actuator Control (TAC) System - Forced Engine Shutdown | ECM | DTC P2105
P2107 | Throttle Actuator Control (TAC) Module Internal Circuit | ECM | DTC P2107 for the 2.4L engine or DTC P2107 for the 2.8L, 3.2L, or 3.6L engine
P2119 | Throttle Closed Position Performance | ECM | DTC P0638, P2100, P2101, or P2119 for the 2.4L engine or DTC P0638, P2100, P2101, or P2119 for the 2.8L, 3.2L, or 3.6L engine
P2120 | Accelerator Pedal Position (APP) Sensor 1 Circuit | ECM | DTC P2120, P2125, or P2138
P2121 | Accelerator Pedal Position (APP) Sensor 1 Performance | ECM | DTC P2121, P2122, P2123, P2127, P2128, or P2138
P2122 | Accelerator Pedal Position (APP) Sensor 1 Circuit Low Voltage | ECM | DTC P2121, P2122, P2123, P2127, P2128, or P2138 for the 2.4L engine or DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.2L, or 3.6L engine
P2123 | Accelerator Pedal Position (APP) Sensor 1 Circuit High Voltage | ECM | DTC P2121, P2122, P2123, P2127, P2128, or P2138 for the 2.4L engine or DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.2L, or 3.6L engine
P2125 | Accelerator Pedal Position (APP) Sensor 2 Circuit Voltage Below Threshold | ECM | DTC P2120, P2125, or P2138
P2127 | Accelerator Pedal Position (APP) Sensor 2 Circuit | ECM | DTC P2121, P2122, P2123, P2127, P2128, or P2138 for the 2.4L engine or DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.2L, or 3.6L engine
P2128 | Accelerator Pedal Position (APP) Sensor 2 Circuit High Voltage | ECM | DTC P2121, P2122, P2123, P2127, P2128, or P2138 for the 2.4L engine or DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.2L, or 3.6L engine
P2135 | Throttle Position (TP) Sensor 1-2 Correlation | ECM | DTC P0121, P0122, P0123, P0221, P0222, P0223, or P2135
P2138 | Accelerator Pedal Position (APP) Sensor 1-2 Correlation | ECM | DTC P2120, P2125, or P2138 for the 2.0L engine or DTC P2122, P2123, P2127, P2128, or P2138 for the 2.4L engine
P2146 | Injector Positive Voltage Control Circuit Group 1 | ECM | DTC P2146 or P2149
P2149 | Injector Positive Voltage Control Circuit Group 2 | ECM | DTC P2146 or P2149
P2176 | Minimum Throttle Position Not Learned | ECM | DTC P2176 for the 2.4L engine or DTC P2176 for the 2.8L, 3.2L, or 3.6L engine
P2177 | Fuel Trim System Lean at Cruise or Accel Bank 1 | ECM | DTC P2177, P2187, or P2191 for the 2.4L engine or DTC P2177, P2179, P2187, or P2189 for the 2.8L, 3.2L, or 3.6L engine
P2178 | Fuel Trim System Rich at Cruise or Accel Bank 1 | ECM | DTC P2178, P2188, or P2192 for the 2.4L engine or DTC P2178, P2180, P2188, or P2190 for the 2.8L, 3.2L, or 3.6L engine
P2179 | Fuel Trim System Lean at Cruise or Accel Bank 2 | ECM | DTC P2177, P2179, P2187, or P2189
P2180 | Fuel Trim System Rich at Cruise or Accel Bank 2 | ECM | DTC P2178, P2180, P2188, or P2190
P2187 | Fuel Trim System Lean at Idle Bank 1 | ECM | DTC P2177, P2187, or P2191 for the 2.4L engine or DTC P2177, P2179, P2187, or P2189 for the 2.8L, 3.2L, or 3.6L engine
P2188 | Fuel Trim System Rich at Idle Bank 1 | ECM | DTC P2178, P2188, or P2192 for the 2.4L engine or DTC P2178, P2180, P2188, or P2190 for the 2.8L, 3.2L, or 3.6L engine
P2189 | Fuel Trim System Lean at Idle Bank 2 | ECM | DTC P2177, P2179, P2187, or P2189
P2190 | Fuel Trim System Rich at Idle Bank 2 | ECM | DTC P2178, P2180, P2188, or P2190
P2191 | Fuel Trim System Lean at Higher Load | ECM | DTC P2177, P2187, or P2191
P2192 | Fuel Trim System Rich at Higher Load | ECM | DTC P2178, P2188, or P2192
P2195 | HO2S Signal Biased Lean Bank 1 Sensor 1 | ECM | DTC P2195 or P2197
P2196 | HO2S Signal Biased Rich Bank 1 Sensor 1 | ECM | DTC P2196 or P2198
P2197 | HO2S Signal Biased Lean Bank 2 Sensor 1 | ECM | DTC P2195 or P2197
P2198 | HO2S Signal Biased Rich Bank 2 Sensor 1 | ECM | DTC P2196 or P2198
P2226 | Barometric Pressure (BARO) Sensor Circuit | ECM | DTC P2226, P2228, or P2229
P2227 | Barometric Pressure (BARO) Sensor Performance | ECM | DTC P2227, P2228, or P2229
P2228 | Barometric Pressure (BARO) Sensor Circuit Low Voltage | ECM | DTC P2226, P2228, or P2229 for the 2.0L engine or DTC P2227, P2228, or P2229 for the 2.8L, 3.2L, or 3.6L engine
P2229 | Barometric Pressure (BARO) Sensor Circuit High Voltage | ECM | DTC P2226, P2228, or P2229 for the 2.0L engine or DTC P2227, P2228, or P2229 for the 2.8L, 3.2L, or 3.6L engine
P2231 | HO2S Signal Circuit Shorted to Heater Circuit Bank 1 Sensor 1 | ECM | DTC P2231 or P2234
P2232 | HO2S Signal Circuit Shorted to Heater Circuit Bank 1 Sensor 2 | ECM | DTC P2232 or P2235
P2234 | HO2S Signal Circuit Shorted to Heater Circuit Bank 2 Sensor 1 | ECM | DTC P2231 or P2234
P2235 | HO2S Signal Circuit Shorted to Heater Circuit Bank 1 Sensor 2 | ECM | DTC P2232 or P2235
P2237 | HO2S Pumping Current Control Circuit Bank 1 Sensor | ECM | DTC P2237 or P2240
P2240 | HO2S Pumping Current Control Circuit Bank 2 Sensor 1 | ECM | DTC P2237 or P2240
P2243 | HO2S Reference Voltage Circuit Bank 1 Sensor 1 | ECM | DTC P2243 or P2247
P2243 | HO2S Reference Voltage Circuit Bank 2 Sensor 1 | ECM | DTC P2243 or P2247
P2251 | HO2S Reference Ground Circuit Bank 1 Sensor 1 | ECM | DTC P2251 or P2254
P2254 | HO2S Reference Ground Circuit Bank 2 Sensor 1 | ECM | DTC P2251 or P2254
P2264 | Water in Fuel Sensor Circuit | ECM | DTC P2264
P2270 | HO2S Signal Stuck Lean Sensor 2 | ECM | DTC P2270 for the 2.4L engine or DTC P2270 or P2272 for the 2.8L, 3.2L, or 3.6L engine
P2271 | HO2S Signal Stuck Rich Sensor 2 | ECM | DTC P2271 for the 2.4L engine or DTC P2271 or P2273 for the 2.8L, 3.2L, or 3.6L engine
P2272 | HO2S Signal Stuck Lean Bank 2 Sensor 2 | ECM | DTC P2270 or P2272
P2273 | HO2S Signal Stuck Rich Bank 2 Sensor 2 | ECM | DTC P2271 or P2273
P2293 | Fuel Pressure Regulator Solenoid 2 Control Circuit Performance | ECM | DTC P2293, P2294, P2295, or P2296
P2294 | Fuel Pressure Regulator Solenoid 2 Control Circuit | ECM | DTC P2293, P2294, P2295, or P2296
P2295 | Fuel Pressure Regulator Solenoid 2 Control Circuit Low Voltage | ECM | DTC P2293, P2294, P2295, or P2296
P2296 | Fuel Pressure Regulator Solenoid 2 Control Circuit High Voltage | ECM | DTC P2293, P2294, P2295, or P2296
P2297 | HO2S Performance During Decel Fuel Cut-Off (DFCO) Bank 1 Sensor 1 | ECM | DTC P2297 or P2298
P2298 | HO2S Performance During Decel Fuel Cut-Off (DFCO) Bank 2 Sensor 1 | ECM | DTC P2297 or P2298
P2299 | Brake Pedal Position Accelerator Pedal Position | ECM | DTC P2299
P2300 | Ignition Coil 1 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2301 | Ignition Coil 1 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2303 | Ignition Coil 2 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2304 | Ignition Coil 2 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2306 | Ignition Coil 3 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2307 | Ignition Coil 3 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2309 | Ignition Coil 4 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2310 | Ignition Coil 4 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2312 | Ignition Coil 5 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2313 | Ignition Coil 5 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2315 | Ignition Coil 6 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2316 | Ignition Coil 6 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P244A | Diesel Particulate Filter Differential Pressure Too Low | ECM | DTC P244A, P244B, or P2453
P244B | Diesel Particulate Filter Differential Pressure Too High | ECM | DTC P244A, P244B, or P2453
P244C | Catalyst Temperature Too Low During Regeneration | ECM | DTC P1446, P1447, P244C, or P244D
P244D | Catalyst Temperature Too High During Regeneration | ECM | DTC P1446, P1447, P244C, or P244D
P2452 | Diesel Particulate Filter Differential Pressure Sensor Circuit Voltage | ECM | DTC P2452, P2454, or P2455
P2453 | Diesel Particulate Filter Differential Pressure Sensor Performance | ECM | DTC P244A, P244B, or P2453
P2454 | Diesel Particulate Filter Differential Pressure Sensor Circuit Low Voltage | ECM | DTC P2452, P2454, or P2455
P2455 | Diesel Particulate Filter Differential Pressure Sensor Circuit High Voltage | ECM | DTC P2452, P2454, or P2455
P2463 | Diesel Particulate Filter Soot Accumulation | ECM | DTC P2463
P2500 | Generator L-Terminal Circuit Low Voltage | ECM | DTC P2501
P2501 | Generator L-Terminal Circuit High Voltage | ECM | DTC P2500
P2510 | Engine Controls Ignition Relay Control Circuit | ECM | DTC P068A, P068B, or P2510
P2533 | Ignition 1 Switch Circuit | TCM | DTC P2533
P2534 | Ignition 1 Switch Circuit Low Voltage | TCM | DTC P2534 for the 6T40/6T45 transmission or DTC P2534 for the AF33-5 transmission
P2536 | Ignition Accessory Switch Circuit | ECM | DTC P2536
TCM | DTC P2536
P253F | Engine Oil Life | ECM | DTC P253F
P2544 | Transmission Torque Request Circuit | ECM | DTC P2544
P2610 | Control Module Ignition Off Timer Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 2.8L, 3.2L, or 3.6L engine
P2626 | HO2S Pumping Current Trim Circuit Bank 1 Sensor 1 | ECM | DTC P2626 or P2629
P2629 | HO2S Pumping Current Trim Circuit Bank 2 Sensor 1 | ECM | DTC P2626 or P2629
P2636 | Fuel Transfer Pump Flow Insufficient | ECM | DTC P2636 for the 2.0L engine or DTC P2636 for the 2.4L engine
P2687 | Fuel Heater Relay Control Circuit | ECM | DTC P2687
P268A | Fuel Injector Calibration Data Not Programmed | ECM | DTC P268A
P2714 | Clutch Pressure Control (PC) Solenoid 4 - Stuck Off | TCM | DTC P2714 or P2715
P2715 | Clutch Pressure Control (PC) Solenoid 4 - Stuck On | TCM | DTC P2714 or P2715
P2719 | Clutch Pressure Control (PC) Solenoid 4 System Performance | TCM | DTC P2719-P2721
P2720 | Clutch Pressure Control (PC) Solenoid 4 Control Circuit Low Voltage | TCM | DTC P2719-P2721
P2721 | Clutch Pressure Control (PC) Solenoid 4 Control Circuit High Voltage | TCM | DTC P2719-P2721
P2723 | Clutch Pressure Control (PC) Solenoid 5 - Stuck Off | TCM | DTC P2723 or P2724
P2724 | Clutch Pressure Control (PC) Solenoid 5 - Stuck On | TCM | DTC P2723 or P2724
P2728 | Clutch Pressure Control (PC) Solenoid 5 System Performance | TCM | DTC P2728-P2730
P2729 | Clutch Pressure Control (PC) Solenoid 5 Control Circuit Low Voltage | TCM | DTC P2728-P2730
P2730 | Clutch Pressure Control (PC) Solenoid 5 Control Circuit High Voltage | TCM | DTC P2728-P2730
P2762 | Torque Converter Clutch (TCC) Pressure Control Solenoid System Performance | TCM | DTC P2762, P2763, or P2764
P2763 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P2762, P2763, or P2764
P2764 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P2762, P2763, or P2764
P280A | Transmission Range (TR) Switch Circuit Not Learned | TCM | DTC P280A
U0073 | Control Module Communication Bus Off | BCM | DTC U0073
U0100 | Lost Communication With ECM A | BCM | DTC U0100-U0299 or U2105-U2199
U0101 | Lost Communication With TCM | BCM | DTC U0100-U0299 or U2105-U2199
U0102 | Lost Communication With Transfer Case Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0104 | Lost Communication With Cruise Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0121 | Lost Communication With ABS Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0122 | Lost Communication With Vehicle Dynamics Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0131 | Lost Communication With Power Steering Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0132 | Lost Communication With Ride Level Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0134 | Lost Communication With Power Steering Control Module - Rear | BCM | DTC U0100-U0299 or U2105-U2199
U0140 | Lost Communication With Body Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0155 | Lost Communication With Instrument Panel Cluster (IPC) Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0158 | Lost Communication With Head Up Display | BCM | DTC U0100-U0299 or U2105-U2199
U0160 | Lost Communication With Audible Alert Control | BCM | DTC U0100-U0299 or U2105-U2199
U0164 | Lost Communication With Body Control Module (BCM) | BCM | DTC U0100-U0299 or U2105-U2199
U0168 | Lost Communication With Vehicle Security Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0184 | Lost Communication With Radio | BCM | DTC U0100-U0299 or U2105-U2199
U0186 | Lost Communication With Audio Amplifier | BCM | DTC U0100-U0299 or U2105-U2199
U0198 | Lost Communication With Telematic Control Module | BCM | DTC U0100-U0299 or U2105-U2199
U0199 | Lost Communication With Door Control Module A | BCM | DTC U0100-U0299 or U2105-U2199
U0200 | Lost Communication With Door Control Module B | BCM | DTC U0100-U0299 or U2105-U2199
U0201 | Lost Communication With Door Control Module C | BCM | DTC U0100-U0299 or U2105-U2199
U0202 | Lost Communication With Door Control Module D | BCM | DTC U0100-U0299 or U2105-U2199
U0214 | Lost Communication With Remote Function Actuation | BCM | DTC U0100-U0299 or U2105-U2199
U0230 | Lost Communication With Rear Gate Module | BCM | DTC U0100-U0299 or U2105-U2199
U0240 | Lost Communication With Headlamp Control Module A | BCM | DTC U0100-U0299 or U2105-U2199
U1814 | Powertrain High Speed Communication Enable Circuit | BCM | DTC U1814
U2099 | High Speed Communication Enable Circuit | BCM | DTC U2099
U2100 | Controller Area Network (CAN) Bus Communication | BCM | DTC U2100
U2101 | Maximum List Of CAN Control Modules Not Programmed | BCM | DTC U2101
U2105 - U2199 | Lost Communication | BCM | DTC U0100-U0299 or U2105-U2199