For 1990-2009 cars

#### Special Tools

• | EN-45059 Torque Angle Sensor Kit

• | EN-48249 Piston Ring Compressor

For equivalent regional tools, refer to Special Tools .

1. Turn the piston rings before the installation to a position (A, B, C) as in the graphic shown.
2. The markings (1) on piston head must point to the timing side.
3. Lubricate the piston rings, piston (1), inner cylinder bore surface and EN-48249 compressor (2) with clean engine oil.
4. Install the 4 pistons with 4 connecting rods (1) push down into the engine block.
5. Install the connecting rod bearings (4) to the connecting rod bearing caps (2).

Note: Take extreme care to prevent any scratches or damages to the connecting rod bearings.

6. Install the 8 connecting rod bearings (4).

Caution: Refer to Fastener Caution in the Preface section.

7. Install the 8 connecting rod bearing cap bolts (3) and tighten in two passes:

7.1. | In first pass tighten to 25 N·m (19 lb ft)

7.2. | In second pass tighten to 90 degrees using the EN-45059 angle sensor .