For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the lamp. Refer to Headlamp Replacement .
3. Twist and remove the bulbs from the headlamp.

### Installation Procedure

1. Insert and twist to install the replacement bulb into the headlamp.
2. Connect the electrical connector.
3. Install the headlamp. Refer to Headlamp Replacement .
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .