For 1990-2009 cars

## Door Check Link Replacement C100/Long Body

### Removal Procedure

1. Remove the door water deflector. Refer to Door Water Deflector Replacement.
2. Remove the bolts on the door and on the body.
3. Remove the door hold-open link.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the door hold-open link to the door and the body with the bolts. Tighten the door hold-open link-to-body bolt to 20 N·m (15 lb ft). Tighten the door hold-open link-to-door bolts to 9 N·m (80 lb in).
2. Install the door water deflector. Refer to Door Water Deflector Replacement.

## Door Check Link Replacement C105/Short Body

### Removal Procedure

1. Remove the door water deflector. Refer to Door Water Deflector Replacement.
2. Remove the bolts on the door and on the body.
3. Remove the door hold-open link.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the door hold-open link to the door and the body with the bolts. Tighten the door hold-open link-to-body bolt to 20 N·m (15 lb ft). Tighten the door hold-open link-to-door bolts to 7 N·m (62 lb in).
2. Install the door water deflector. Refer to Door Water Deflector Replacement.