For 1990-2009 cars

### Removal Procedure

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.
2. Remove the bolts and the rear impact bar.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the rear impact bar with the bolts and tighten to 22 N·m (16 lb ft).
2. Install the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.