For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel lower trim panel. Refer to Instrument Panel Lower Trim Panel Replacement - Left Side.
2. Remove the knee bolster. Refer to Knee Bolster Replacement.
3. Remove the stop lamp switch. Refer to Stop Lamp Switch Replacement.
4. Disconnect the retaining clip from the pushrod of brake booster.
5. Remove the nut and the bolt from the top of brake pedal arm.
6. Remove the brake pedal.
7. Remove the brake pedal cover from the brake pedal.

### Installation Procedure

1. Install the brake pedal cover to the brake pedal.
2. Coat the brake pedal arm with grease.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the bolt and the nut to the top of brake pedal arm and tighten to 18 N·m (13 lb ft).
4. Install the retaining clip to the pushrod of the booster.
5. Install the stop lamp switch. Refer to Stop Lamp Switch Replacement.
6. Install the knee bolster. Refer to Knee Bolster Replacement.
7. Install the instrument panel lower trim panel. Refer to Instrument Panel Lower Trim Panel Replacement - Left Side.