For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the front tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
3. Remove the front brake rotor. Refer to Front Brake Rotor Replacement .
4. Disconnect the wheel speed sensor electrical connector, if equipped.
5. Remove the wheel speed sensor electrical connector, if equipped, from the connector bracket.
6. Remove the front hub nut.
7. Support the wheel drive shaft with heavy mechanic's wire or equivalent.
8. Remove and discard the wheel bearing/hub mounting bolts.
9. Remove the wheel bearing/hub assembly from the steering knuckle.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the wheel bearing/hub assembly to the steering knuckle with the bolts.

Tighten
Tighten the hub to knuckle bolts to 115 N·m (85 lb ft).

2. Install the hub nut to the axle shaft.

Tighten
Tighten the hub nut to 205 N·m (157 lb ft).

3. Remove the mechanic's wire from the wheel drive shaft.
4. Install the wheel speed sensor electrical connector, if equipped, to the mounting bracket.
5. Connect the wheel speed sensor electrical connector, if equipped.
6. Install the front brake rotor. Refer to Front Brake Rotor Replacement .
7. Install the front tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
8. Lower the vehicle.