For 1990-2009 cars

#### Tools Required

J 36346 Fascia Retainer Remover

### Adjustment Procedure

1. Apply the parking brake and ensure the vehicle is not running.
2. Ensure that the shift control assembly is in the park (P) position.
3. Pull back the white plastic cover (1) on the center connector.
4. Pull up on the center tabs of the lock button (2).

Important: This step must be performed correctly to avoid a misadjusted cable. Do not grasp the shift cable end (2) during this procedure.

5. Release the shift cable end (2) and allow the blue spring to tension/adjust the shift cable system.
6. Pull the white cover (3) on the shift cable end (1) back.
7. Push the natural colored lock button (2) down to engage the locking teeth on the shift cable end (1).
8. Release the white cover (1).
9. Verify the white cover (1) conceals the natural colored lock (2).
10. If the white cover (1) does not conceal the natural colored lock (2), the shift cable must be readjusted.
11. Test the transmission for proper shift operation.
12. If all of the gear positions cannot be achieved, the shift cable must be readjusted.